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NAESB OASIS Standards and Communication Protocol (S&CP) – WEQ 011

Business Practices for Open Access Same-Time Information Systems (OASIS) Implementation Guide
Business Practices Requirements:
011-1
INTRODUCTION
This OASIS Implementation Guide provides supplemental information related to certain transaction processing requirements and related business processes required for OASIS.  The technical standards for OASIS are defined in Standards WEQ 002 and WEQ 003, and the companion business practice standards are defined in Standards WEQ 001.
In the event of a conflict between a Transmission Provider’s Tariff, applicable Business Practices, and this Implementation Guide, the Tariff shall take precedence over all, and Business Practices shall take precedence over this document.
011-1.1
Usage of Terms
The following terms as used throughout this Implementation Guide are to be interpreted as follows:
OASIS – Refers to the Transmission Provider’s implementation of the OASIS Customer interface as defined in Standards WEQ 002, and any back-end supporting systems or user procedures that collectively perform the transaction processing functions associated with handling of requests on OASIS.
Business Practice – Refers collectively to any business practices adopted by the Transmission Provider as defined in their Open Access Transmission Tariff (OATT), NAESB ratified Business Practice Standards, or provider specific practices or requirements.

Template – Refers generically, or by reference to a specifically named template, to the templates defined for the Customer interface to OASIS in Standards WEQ 002, including the displays and forms associated with the web browser based user interface implementing the functions of an OASIS defined template.
Must, shall, or required – Define specific requirements for OASIS processing that are not optional and must be implemented as described.

May, should, or optional – Define optional requirements that are recommended for implementation in OASIS but are not specifically required under these Standards.
Additional terms defined in Standards WEQ 001 and WEQ 002 are also hereby incorporated by reference.
011-2
OASIS TRANSACTION PROCESSING
The basic OASIS transaction process is specified in WEQ 002-4.2.10.  The following Standards provide additional guidance for processing specific types of business transactions in the implementation of OASIS.  Note that the (Primary) Transmission Provider may, but is not limited to, interacting with OASIS using the Transmission Customer template or user interface.  Transmission Providers may also implement OASIS functions on back-end systems and are not required to perform all transaction processing on an OASIS node proper, provided that the results of all transaction processing are correctly posted on OASIS as required by the Tariff, regulation, or other established business practices.

011-2.1
Basic OASIS Request Processing
Requests to reserve or purchase transmission or ancillary service shall be submitted to OASIS by the Transmission Customer via the transrequest or ancrequest templates.
The Seller specified in the request must be the Primary Transmission Provider for REQUEST_TYPEs of ORIGINAL, REDIRECT, RELINQUISH, RENEWAL, or DEFERRAL.  The Seller specified in the request must be a registered entity other than the Transmission Provider for REQUEST_TYPE of RESALE or TRANSFER.  The Seller may be either the Transmission Provider or another registered entity for REQUEST_TYPEs of RECALL or MATCHING.  
OASIS should screen submitted requests to validate proper use of REQUEST_TYPE.  Additional restrictions based on specific  REQUEST_TYPEs are detailed in subsequent Standards.  Validations on the service requested, service start time and duration, submission time, etc., are established by business practice.
Once successfully submitted on OASIS, the Seller may take any of the following actions via the transsell/ancsell template:

· Acknowledge receipt by setting STATUS to RECEIVED or STUDY

· Deny the request by setting STATUS to INVALID, DECLINED, or REFUSED

· Approve the request by setting STATUS to ACCEPTED or COUNTEROFFER

At any time during the processing of the request, the Customer may set STATUS to WITHDRAWN to remove the request from further consideration by the Seller.

Once the Seller approves the request, the Customer may take any of the following actions via the transcust/anccust template:
· WITHDRAW the request

· Continue negotiation of the request by setting STATUS to REBID

· Complete the request by setting STATUS to CONFIRMED

Prior to final confirmation by the Customer, the Seller may override their approval of the request with the following actions:

· Retract approval based on exceeding of customer confirmation time limits and/or scheduling deadlines or other criteria established by business practice by setting the STATUS to RETRACTED

· Retract approval based on receipt of a higher priority competing request by setting the STATUS to SUPERSEDED

Once CONFIRMED on OASIS by the Customer a service reservation shall be deemed to exist.  The Seller or the Transmission Provider may take the following actions on a CONFIRMED service reservation:

· Nullify the reservation for cause by setting the STATUS to ANNULLED

· Displace the reservation in-whole to accommodate a higher priority competing request by setting the STATUS to DISPLACED

Seller’s shall provide a reason in the SELLER_COMMENTS whenever a service request is set to the STATUS of INVALID, REFUSED, DECLINED, RETRACTED, SUPERSEDED, ANULLED or DISPLACED.  The Transmission Provider, when not acting as the Seller, shall provide a reason in the PROVIDER_COMMENTS whenever a service request is set to the STATUS of ANNULLED or DISPLACED.
011-2.2
Offering of Partial Service

If in the evaluation of a transmission request, the Primary Transmission Provider determines that only a portion of the Customer's requested capacity (CAPACITY_REQUESTED Data Element) can be accommodated and that the Provider is obligated or elects to offer the Customer only a portion of the requested capacity, the Primary Provider shall set the CAPACITY_GRANTED Data Element associated with that transmission service request to the amount available, and set the request’s STATUS to COUNTEROFFER. 
If the CAPACITY_REQUESTED and/or CAPACITY_GRANTED are not constant over time, continuation records shall be used to convey the time varying profile of MW capacity associated with the transmission request via the Data Elements CAPACITY_REQUESTED, CAPACITY_GRANTED, START_TIME and STOP_TIME.  The profile of CAPACITY_GRANTED must span the entire START_TIME to STOP_TIME interval initially requested by the Customer even if CAPACITY_GRANTED is zero.
The Customer shall recognize the offer of partial service by CAPACITY_REQUESTED not being equal to CAPACITY_REQUESTED and the request STATUS of COUNTEROFFER. The Customer may elect to CONFIRM, WITHDRAW, or REBID the reservation using the transcust Template.  
If the transmission reservation request was marked PRECONFIRMED by the Customer and an offer of partial service is extended, the reservation request must be explicitly CONFIRMED by the Customer.  The OASIS node shall not automatically confirm a request where CAPACITY_REQUESTED does not equal CAPACITY_GRANTED when/if the request STATUS is set to ACCEPTED.

011-2.3
Negotiation of Price
Negotiation of price is initiated by the Customer submitting a service request (via transrequest/ancrequest) with a BID_PRICE that is different from the currently posted offer price, or the tariff rate, for that service.  The following negotiation process is required where the Seller is the Primary Transmission Provider.  Resales or transfers between Transmission Customers may use this process, but there is no obligation on the (Re)Seller to offer a negotiated rate to other Customers.
If the Seller determines that the BID_PRICE is acceptable, the following actions must be taken (via transsell/ancsell):

· Update the currently posted offer price for the service requested and all other applicable services offered as dictated by current discounting policy (e.g., all unconstrained paths to the same point of delivery) to match BID_PRICE;

· Update the request’s NEGOTIATED_PRICE_FLAG to ‘L’ or ‘H’ if the BID_PRICE was lower than or higher than, respectively, the posted price when the request was submitted;
· Set the OFFER_PRICE equal to the BID_PRICE;

· Set the CAPACITY_GRANTED appropriately (if left null or undefined, OASIS shall set CAPACITY_GRANTED equal to CAPACITY_REQUESTED when STATUS is set to ACCEPTED);

· Set the request STATUS to ACCEPTED (or COUNTEROFFER if offering partial service)

The Customer may then confirm the purchase or withdraw the request by updating the request STATUS (via transcust/anccust).

If the Seller determines that the BID_PRICE is unacceptable, and negotiation of price is not going to be entertained, the Seller shall set the request STATUS to DECLINED (via transsell/ancsell):

If the Seller elects to enter into price negotiation, the following actions must be taken (via transsell/ancsell):
· If the price to be counter offered to the Customer is different than the currently posted offer price:

· Update the currently posted offer price for the service requested and all other applicable services offered as dictated by current discounting policy (e.g., all unconstrained paths to the same point of delivery) to match the price to be counteroffered;

· Update the request’s NEGOTIATED_PRICE_FLAG to ‘L’ or ‘H’ if the price to be counter offered is lower than or higher than, respectively, the posted price when the request was submitted;

· Set the OFFER_PRICE and CAPACITY_GRANTED appropriately;
· Set the request STATUS to COUNTEROFFER.
The Customer may then confirm the purchase, withdraw the request, or propose a new BID_PRICE by performing the following (via transcust/anccust):

· Update the request BID_PRICE;

· Set the request STATUS to REBID.

The Seller may then act on the new BID_PRICE by declining the request, accepting the BID_PRICE, or counter offering a new OFFER_PRICE using the same sequence of actions as stated above.

Negotiation of price may also be initiated on receipt of a request for similar service submitted with a higher BID_PRICE.  If required by business practice, the Seller (Primary Transmission Provider) may update any ACCEPTED but unconfirmed requests to COUNTEROFFER with the associated OFFER_PRICE set to meet the higher received BID_PRICE, and the negotiation of price can proceed as described above.
011-2.4
Displacement – No Right of First Refusal

Confirmed transmission reservations may be subject to displacement in the event competing, higher priority requests are received by the Primary Transmission Provider. 
If the existing Customer does not have the right of first refusal and all capacity from that Customer’s confirmed reservation is required to accommodate the higher priority request, the Primary Transmission Provider shall set the existing reservation's STATUS to DISPLACED. The STATUS of DISPLACED indicates that the reservation has been displaced in its entirety. 
If only a portion of the confirmed reservation's capacity is required to accommodate the higher priority request, the Primary Transmission Provider shall document the "recall" of reserved capacity from the lower priority confirmed reservation by incrementing the IMPACTED counter on that reservation and posting on OASIS the amount and time frames over which that reservation's capacity was reduced, i.e., a partial displacement. The Transmission Customer may view all impacts to existing transmission service reservations (e.g., partial displacements, secondary sales, etc.) using the reduction Template. 

A reference to the competing transmission service request that forced the displacement should be entered in the SELLER_COMMENTS field of the displaced reservation.
011-2.5
Displacement – With Right of First Refusal

[ed: Note that this section is subject to potential major revision as standards for competition and displacement are drafted.]

Confirmed transmission reservations may be subject to displacement in the event competing, higher priority requests are received by the Primary Transmission Provider, but have the right of first refusal to retain their transmission service.

If the Primary Provider's Tariff obligates, or the Primary Provider elects to grant the original Customer the right of first refusal, the existing Customer shall be notified of the competing request. The Primary Provider shall set the existing lower priority reservation's COMPETING_REQUEST_FLAG to Y and update the SELLER_COMMENTS to include the ASSIGNMENT_REF associated with the higher priority competing request. These actions will initiate electronic notification, provided the Customer has elected to receive such notification.  
If the existing Customer elects to meet the terms and conditions of the competing request,  that Customer shall submit a new MATCHING reservation request using the transrequest template.  The specific requirements associated with submission of MATCHING requests are detailed in Standard 001-2.x.

If the Primary Provider accepts and the Customer confirms the MATCHING request, the Primary Provider shall set the STATUS of the competing request to "REFUSED" and set the STATUS of the existing lower priority confirmed reservation to "DISPLACED". The STATUS of DISPLACED indicates that the reservation has been displaced in its entirety and has been replaced by the confirmed MATCHING reservation.  
If the existing Customer does not elect to meet the terms of the competing request, the Primary Transmission Provider shall displace the existing lower priority reservation, in whole or in part, in the same manner described for displacement of reservations that are not extended a right of first refusal.  
Once the result of the competition is resolved, whether through MATCHING or displacement of the existing reservation, the Transmission Provider shall reset the COMPETING_REQUEST_FLAG to "N" in the reservation subject to displacement. 

011-2.6
Provider Recalls
There are cases in implementing provisions of the Primary Transmission Provider's Tariff that the capacity reserved by a Transmission Customer may be reduced in whole or in part. The particular reasons for these reductions are Tariff specific. 
The Transmission Provider shall provide a mechanism to post on OASIS any such reductions or "recalls" in reserved capacity. The Customer shall be notified of any and all such reductions in reserved capacity by the incrementing of the IMPACTED counter in association with those reservations that are reduced; the IMPACTED flag is viewable with the transstatus template.  Specific information regarding the exact nature of each reduction in the reserved capacity under a given transmission reservation shall be posted and viewable with the reduction template.

A specific example of a Primary Provider initiated recall of reserved capacity is the implementation of a partial displacement of a transmission reservation. In this instance, the Customer has not elected (or was not required to be offered) to match the terms of a higher priority, competing request. The Primary Transmission Provider "recalls" that capacity necessary to accommodate the higher priority request from the existing lower priority reservation. The IMPACTED counter of that reservation is incremented, and a query using the reduction template for that reservation would show the Customer the amount and time-frame over which the Customer's reserved capacity was recalled by the Primary Provider.

Interruption of transmission service, where that interruption directly impacts the rights of the Customer to schedule any service under that reservation, is another example of an impact to reserved capacity that would be posted as a Primary Transmission Provider initiated recall of reserved capacity.   Secondary market sales of transmission rights are not examples of a Provider initiated recall of reserved capacity, but the impact of any such sales shall also be returned in response to execution of the reduction Template.
The Transmission Provider may elect to post recalls of reserved capacity using the OASIS RECALL request.  Documenting Transmission Provider initiated recalls of capacity with a RECALL request is optional; posting the results of those recalls to be made available under the reduction template is mandatory.  If the RECALL request is used by the Transmission Provider, its use must be implemented in compliance with the Standards for RECALL requests.

011-2.7
ORIGINAL Requests
ORIGINAL requests shall be submitted by the Customer to arrange for new transmission or ancillary service with the Primary Transmission Provider.
The following are specific restrictions or requirements for OASIS service requests with REQUEST_TYPE of ORIGINAL.  If REQUEST_TYPE is not specified by the Customer and SELLER_CODE and SELLER_DUNS are the same as PRIMARY_PROVIDER_CODE and PRIMARY_PROVIDER_DUNS, OASIS shall default REQUEST_TYPE to ORIGINAL.

	Data Element
	Restriction/Requirement

	REQUEST_TYPE
	Must be ORIGINAL

	RELATED_REF
	Must be null

	SELLER_CODE
	Must match PRIMARY_PROVIDER_CODE

	SELLER_DUNS
	Must match PRIMARY_PROVIDER_DUNS


Additional requirements related to the specification of service points, attributes, pricing, and timing are subject to the Transmission Provider’s business practices.

011-2.8
RENEWAL Requests
Transmission Customers shall use the RENEWAL request to exercise their on-going renewal or rollover rights associated with an existing transmission service reservation held by the Customer.  RENEWAL requests must always specify the Primary Transmission Provider as SELLER.

The following are specific restrictions or requirements for OASIS service requests with REQUEST_TYPE of RENEWAL.

	Data Element
	Restriction/Requirement

	REQUEST_TYPE
	Must be RENEWAL

	RELATED_REF
	Must specify the ASSIGNMENT_REF associated with an existing confirmed transmission service reservation held by the Customer that 1) has renewal/rollover rights, and 2) whose renewal/rollover rights have not expired. 

	SELLER_CODE
	Must match PRIMARY_PROVIDER_CODE

	SELLER_DUNS
	Must match PRIMARY_PROVIDER_DUNS

	PATH
	Must represent the same corresponding service points in the reservation specified in RELATED_REF

	POINT_OF_RECEIPT
	

	POINT_OF_DELIVERY
	

	SOURCE
	

	SINK
	

	SERVICE_INCREMENT
	Must specify a set of valid transmission service attributes recognized by the Transmission Provider as a valid service designation eligible for exercising of renewal/rollover rights held by the reservation specified in RELATED_REF

	TS_CLASS
	

	TS_TYPE
	

	TS_PERIOD
	

	TS_WINDOW
	

	TS_SUBCLASS
	

	START_TIME
	Must match the STOP_TIME of the reservation specified in RELATED_REF 

	STOP_TIME
	With START_TIME, must specify a valid interval of service eligible for exercising of renewal/rollover rights held by the reservation specified in RELATED_REF

	CAPACITY_REQUESTED
	Must be less than or equal to the amount of capacity eligible for renewal/rollover over the interval of service


RENEWAL requests must be submitted on OASIS prior to expiration of the Customer’s renewal/rollover rights as established by business practice, e.g., 60 days prior to end of service.

The transmission service attributes, e.g., TS_CLASS, etc., should match the corresponding attributes in the reservation specified in RELATED_REF.  However, changes may be made to these attributes over time such that some differences are necessary to accommodate changes in the Provider’s business practices.  This also applies to changes in service points, e.g., PATH, etc., over time.

011-2.9
DEFERRAL Requests
[ed: We have a basic question to address with this request type.  Should the result be a modification to the original reservation (like RELINQUISH and RECALL), or should the DEFERRAL totally replace and be used instead of the original reservation (like REDIRECT and RENEWAL)?  Its currently written as the latter.]

The DEFERRAL request shall be used by Transmission Customers to request a delay in the start of an existing transmission service reservation held by the Customer.  Transmission Providers may use a DEFERRAL request to document the deferral of the start of service due to the need to complete necessary system studies before approval of a transmission service request.  
DEFERRAL requests must always specify the Primary Transmission Provider as SELLER.

The following are specific restrictions or requirements for OASIS service requests with REQUEST_TYPE of DEFERRAL.

	Data Element
	Restriction/Requirement

	REQUEST_TYPE
	Must be DEFERRAL

	RELATED_REF
	If submitted by the Customer, must specify the ASSIGNMENT_REF associated with an existing confirmed transmission service reservation held by the Customer whose start time is to be delayed/deferred.

If posted by the Transmission Provider, must specify the ASSIGNMENT_REF associated with a pending transmission service request submitted by the Customer whose start time is to be deferred.



	SELLER_CODE
	Must match PRIMARY_PROVIDER_CODE

	SELLER_DUNS
	Must match PRIMARY_PROVIDER_DUNS

	PATH
	Must represent the same corresponding service points in the reservation/request specified in RELATED_REF

	POINT_OF_RECEIPT
	

	POINT_OF_DELIVERY
	

	SOURCE
	

	SINK
	

	SERVICE_INCREMENT
	Must represent the same set of valid transmission service attributes recognized by the Transmission Provider as a valid service designation specified in the reservation/request specified in RELATED_REF

	TS_CLASS
	

	TS_TYPE
	

	TS_PERIOD
	

	TS_WINDOW
	

	TS_SUBCLASS
	

	START_TIME
	Must specify the new requested time for the start of transmission service and must be greater than the START_TIME of the reservation/request specified in RELATED_REF 

	STOP_TIME
	With START_TIME, must specify a valid interval of service based on the transmission service attributes

	CAPACITY_REQUESTED
	Must be equivalent to the amount of capacity originally reserved/requested


When submitted by the Transmission Customer and ultimately approved and confirmed, OASIS or the Transmission Provider procedurally must set the status of the reservation specified in RELATED_REF to ANNULLED.  The DEFERRAL request becomes the new transmission service reservation reflecting the delay in start of service requested.

If the DEFERRAL is posted by the Transmission Provider to reflect deferral of start of service due to delays in completing necessary studies,  OASIS or the Transmission Provider procedurally must set the status of the reservation specified in RELATED_REF to SUPERSEDED.  The DEFERRAL request becomes the new transmission service request reflecting the new expected start of service.  The Transmission Provider shall evaluate pending DEFERRAL requests relative to other transmission requests based on the TIME_QUEUED of the Customer’s ORIGINAL request for service.
011-2.10
RESALE Requests

RESALE requests may be submitted by the Customer (Assignee) to arrange for the sale or assignment of scheduling rights from another Transmission Customer (Reseller). Resellers and Assignees are not obligated to use OASIS to arrange for such sale or assignment of scheduling rights.  However, the Reseller is obligated/required to notify the Primary Transmission Provider and post information documenting the (re)sale on the Provider’s OASIS where the rights were originally acquired.

The following are specific restrictions or requirements for OASIS service requests with REQUEST_TYPE of RESALE.  If REQUEST_TYPE is not specified by the Customer and SELLER_CODE and SELLER_DUNS are not the same as PRIMARY_PROVIDER_CODE and PRIMARY_PROVIDER_DUNS, OASIS shall default REQUEST_TYPE to RESALE.
011-2.10.1
RESALE on OASIS

Resale transactions conducted on OASIS shall adhere to the Basic OASIS Request Processing requirements where the Reseller is identified as the Seller and the Assignee identified as the Customer.  

The Assignee (Customer) initiates the resale of scheduling rights by submitting the following required information on OASIS via the transrequest template.  Data elements not listed are optional There shall be no requirement imposed by OASIS that the Reseller has or has not posted any corresponding offer of service for sale on that OASIS.

	Data Element
	Restriction/Requirement

	REQUEST_TYPE
	Must be RESALE

	RELATED_REF
	Must be null

	SELLER_CODE
	Must identify the Reseller (registered entity other than the Primary Transmission Provider)

	SELLER_DUNS
	Must identify the Reseller

	PATH
	Must represent the transmission service points being requested

	POINT_OF_RECEIPT
	

	POINT_OF_DELIVERY
	

	SOURCE
	

	SINK
	

	SERVICE_INCREMENT
	Must represent a set of valid transmission service attributes offered by the Primary Transmission Provider and being requested from the Reseller

	TS_CLASS
	

	TS_TYPE
	

	TS_PERIOD
	

	TS_WINDOW
	

	TS_SUBCLASS
	

	START_TIME
	Must specify the requested start of transmission service 

	STOP_TIME
	Must specify the requested stop/end of transmission service 

	CAPACITY_REQUESTED
	Must specify the amount of transmission capacity being requested

	BID_PRICE
	Should specify the price being requested; may be null


If the RESALE meets all OASIS validation requirements, the RESALE request shall be posted on OASIS as a QUEUED transmission service request.  It is the Reseller’s obligation to respond to RESALE requests submitted to them on OASIS.  Resellers may register for dynamic notification of these events if the Primary Transmission Provider’s OASIS implementation provides for such functionality.

The Reseller may act on the RESALE request using any of the processes defined for Basic OASIS Request Processing, Offering of Partial Service, and/or Negotiation of Price.  At some point in this process, the Reseller must identify those transmission service reservations whose scheduling rights are to be conferred to the Assignee as follows.

	Data Element
	Restriction/Requirement

	REASSIGNED_REF
	Collectively represent those confirmed transmission reservations held by the Reseller whose rights to schedule transmission capacity over time are to be conferred to the Assignee.  Each reservation’s service points and transmission service attributes must correspond with those specified in the  RESALE request

	REASSIGNED_CAPACITY
	

	REASSIGNED_START_TIME
	

	REASSIGNED_STOP_TIME
	


OASIS or Transmission Provider business practice may dictate that this information be supplied and validated at the time the RESALE request STATUS is set to either ACCEPTED or COUNTEROFFER.

Once the RESALE request is finally CONFIRMED by the Assignee, OASIS or Transmission Provider procedures should (again) insure that every reservation represented in the REASSIGNED_REF data element meet the following requirements:

· Represent valid confirmed transmission service reservations held by the Reseller

· There is sufficient unscheduled or otherwise encumbered (e.g., other RESALE, REDIRECT, etc., transactions)  transmission capacity to meet REASSIGNED_CAPACITY over REASSIGNED_START_TIME toi REASSIGNED_STOP_TIME

· Service points, e.g., PATH, etc., correspond correctly with those specified in the RESALE

· Transmission service attributes, e.g., TS_CLASS, etc., correspond correctly with those specified in the RESALE

· The sum of REASSIGNED_CAPACITY over time for all REASSIGNED_REF reservations satisfies the RESALE requirements as specified in CAPACITY_GRANTED, START_TIME and STOP_TIME.

If all of these requirements are met, OASIS or Transmission Provider procedures shall convey the specified transmission rights from the Reseller’s reservation to the Assignee’s reservation.  Unless recalled by the Reseller, the transmission capacity resold shall not be available to the Reseller to schedule, resell, redirect, or otherwise use.

If the Primary Transmission Provider determines the posted RESALE does not comply with their business practices for such transactions, they shall have the right to reset the RESALE STATUS to ANNULLED.  OASIS or Transmission Provider procedures shall then reinstate any and all reassignments of capacity over time that were designated by the Assignee to the parent (REASSIGNED_REF) reservation(s) as appropriate.
011-2.10.2
RESALE off OASIS

Resale transactions arranged between Reseller and Assignee off OASIS must be documented on OASIS by the Reseller using the transassign  template.  Transactions arranged off OASIS do not follow the basic request processing steps and shall be posted directly as CONFIRMED transactions.

The following information is required to be supplied by the Reseller.  
	Data Element
	Restriction/Requirement

	REQUEST_TYPE
	Must be RESALE

	RELATED_REF
	Must be null

	CUSTOMER_CODE
	Must identify the Assignee

	CUSTOMER_DUNS
	Must identify the Assignee

	PATH
	Must represent the same corresponding service points as contained in every one of the reservation/request(s) specified by REASSIGNED_REF

	POINT_OF_RECEIPT
	

	POINT_OF_DELIVERY
	

	SOURCE
	

	SINK
	

	SERVICE_INCREMENT
	Must represent the same corresponding transmission service attributes as contained in every one of the reservation/request(s) specified by REASSIGNED_REF 

	TS_CLASS
	

	TS_TYPE
	

	TS_PERIOD
	

	TS_WINDOW
	

	TS_SUBCLASS
	

	START_TIME
	Must specify the start of transmission service arranged between Reseller and Assignee

	STOP_TIME
	Must specify the stop/end of transmission service arranged between Reseller and Assignee

	CAPACITY_REQUESTED
	Must be equal to the amount of capacity originally reserved/requested by the Assignee

	CAPACITY_GRANTED
	Must be equal to the amount of capacity ultimately resold to the Assignee 

	OFFER_PRICE
	Must be the ultimate price arranged for service between Reseller and Assignee

	REASSIGNED_REF
	Collectively represent those confirmed transmission reservations held by the Reseller whose rights to schedule transmission capacity over time are to be conferred to the Assignee

	REASSIGNED_CAPACITY
	

	REASSIGNED_START_TIME
	

	REASSIGNED_STOP_TIME
	


OASIS or Transmission Provider procedures should insure that every reservation represented in the REASSIGNED_REF data element meet the following requirements:

· Represent valid confirmed transmission service reservations held by the Reseller

· There is sufficient unscheduled or otherwise encumbered (e.g., other RESALE, REDIRECT, etc., transactions)  transmission capacity to meet REASSIGNED_CAPACITY over REASSIGNED_START_TIME toi REASSIGNED_STOP_TIME

· Service points, e.g., PATH, etc., correspond correctly with those specified in the RESALE

· Transmission service attributes, e.g., TS_CLASS, etc., correspond correctly with those specified in the RESALE

· The sum of REASSIGNED_CAPACITY over time for all REASSIGNED_REF reservations satisfies the RESALE requirements as specified in CAPACITY_GRANTED, START_TIME and STOP_TIME.

If all of these requirements are met, OASIS or Transmission Provider procedures shall convey the specified transmission rights from the Reseller’s reservation to the Assignee’s reservation.  Unless recalled by the Reseller, the transmission capacity resold shall not be available to the Reseller to schedule, resell, redirect, or otherwise use.

If the Primary Transmission Provider determines the posted RESALE does not comply with their business practices for such transactions, they shall have the right to reset the RESALE STATUS to ANNULLED.  OASIS or Transmission Provider procedures shall then reinstate any and all reassignments of capacity over time that were designated by the Assignee to the parent (REASSIGNED_REF) reservation(s) if appropriate.
011-2.11
TRANSFER Requests

[ed. We need to decide if we must fully implement a three-way confirmation process by addition of data elements to the transstatus template.  We also have to determine if the TRANSFER transaction itself represents the capacity transferred, or it is handled like RELINQUISH and modifies an existing reservation – like modifying Customer and Seller attributes to match Assignee and TP.  Aside for that these sections will be very similar to RESALE.]

TRANSFER requests may be submitted by the Customer (Assignee) to arrange for the complete transfer of all rights, include all financial obligations to the Primary Transmission Provider, from another Transmission Customer (Reseller). Resellers and Assignees are not obligated to use OASIS to arrange for such sale or assignment of transmission rights. TRANSFER is analogous to RESALE with the following specific requirements:

· The Reseller must be the Customer that originally arranged for the transmission service directly with the Primary Transmission Provider

· All three parties to the TRANSFER, Reseller, Assignee, and Primary Transmission Provider, must agree and approve the transaction

The following are specific restrictions or requirements for OASIS service requests with REQUEST_TYPE of TRANSFER.
011-2.10.1
TRANSFER on OASIS

011-2.10.2
TRANSFER off OASIS

011-2.11
REDIRECT Requests 

The REDIRECT request is submitted by an existing firm point-to-point transmission customer to request the use of alternate points of receipt and/or delivery from the Primary Transmission Provider.  By definition, the Seller in a REDIRECT request must be the Primary Transmission Provider even if those rights being redirected were acquired from another Transmission Customer via Resale or Transfer.

The following Standards set forth the requirements for submission of REDIRECT requests on either a Firm or Non-Firm basis.

011-2.12.1
REDIRECT on a Firm Basis

A Customer holding confirmed firm point-to-point transmission rights may request the use of those rights on alternate points of receipt and/or delivery on a firm basis by submission of a REDIRECT request to the Primary Transmission Provider as Seller.  The following information must be submitted by the customer in the REDIRECT request via the transrequest template.

	Data Element
	Restriction/Requirement

	REQUEST_TYPE
	Must be REDIRECT

	RELATED_REF
	Must identify by ASSIGNMENT_REF a confirmed transmission service reservation for firm point-to-point service held by the submitting Customer

	SELLER_CODE
	Must match PRIMARY_PROVIDER_CODE

	SELLER_DUNS
	Must match PRIMARY_PROVIDER_DUNS

	PATH
	Must represent the new transmission service points being requested

	POINT_OF_RECEIPT
	

	POINT_OF_DELIVERY
	

	SOURCE
	

	SINK
	

	SERVICE_INCREMENT
	Must represent a set of valid transmission service attributes for firm point-to-point service offered by the Primary Transmission Provider and being requested on the new service points by the Customer

	TS_CLASS
	

	TS_TYPE
	

	TS_PERIOD
	

	TS_WINDOW
	

	TS_SUBCLASS
	

	START_TIME
	Must specify the requested start of transmission service and must be within the bounds of START_TIME specified in the reservation identified in RELATED_REF

	STOP_TIME
	Must specify the requested stop/end of transmission service and must be within the bounds of STOP_TIME specified in the reservation identified in RELATED_REF, and with START_TIME must represent a valid interval of service for the firm point-to-point service being requested

	CAPACITY_REQUESTED
	Must specify the amount of transmission capacity being requested

	BID_PRICE
	Should specify the price for the service being requested; may be null


The Primary Transmission Provider shall evaluate each REDIRECT on a Firm basis as any other new request for firm point-to-point transmission service.  Provider business practices establish the requirements for service duration, submission time, evaluation time, confirmation time, etc.

OASIS or Transmission Provider procedures should verify that the transmission reservation identified in RELATED_REF meets all the requirements to support the redirect of transmission rights to the new service points.  This should include the validation that the current rights, the Capacity Available for Redirect, held on that reservation in the amount of the REDIRECT over time have not be encumbered by any other confirmed redirects, resales, schedules, etc.  This capacity validation may occur at any point in the request process, but shall always be performed at the time the REDIRECT STATUS is attempting to be set to CONFIRMED.
Once CONFIRMED, the transmission rights held on the RELATED_REF reservation in the amount of the REDIRECT shall be permanently released by the Transmission Provider and conveyed to the REDIRECT reservation. The only mechanism for the Customer to return to the original points of receipt and/or delivery is to submit another REDIRECT request.

011-2.12.2
REDIRECT on a Non-Firm Basis

A Customer holding confirmed firm point-to-point transmission rights may request the use of those rights on alternate points of receipt and/or delivery on a non-firm basis by submission of a REDIRECT request to the Primary Transmission Provider as Seller.  The following information must be submitted by the customer in the REDIRECT request via the transrequest template.

	Data Element
	Restriction/Requirement

	REQUEST_TYPE
	Must be REDIRECT

	RELATED_REF
	Must identify by ASSIGNMENT_REF a confirmed transmission service reservation for firm point-to-point service held by the submitting Customer

	SELLER_CODE
	Must match PRIMARY_PROVIDER_CODE

	SELLER_DUNS
	Must match PRIMARY_PROVIDER_DUNS

	PATH
	Must represent the new transmission service points being requested

	POINT_OF_RECEIPT
	

	POINT_OF_DELIVERY
	

	SOURCE
	

	SINK
	

	SERVICE_INCREMENT
	Must be HOURLY

	TS_CLASS
	Must be SECONDARY

	TS_TYPE
	Must be POINT_TO_POINT

	TS_PERIOD
	Must be FULL_PERIOD

	TS_WINDOW
	Must be FIXED

	TS_SUBCLASS
	Must be null

	START_TIME
	Must specify the requested start of transmission service and must be within the bounds of START_TIME specified in the reservation identified in RELATED_REF

	STOP_TIME
	Must specify the requested stop/end of transmission service and must be within the bounds of STOP_TIME specified in the reservation identified in RELATED_REF, and with START_TIME must represent a valid interval of service for the firm point-to-point service being requested

	CAPACITY_REQUESTED
	Must specify the amount of transmission capacity being requested

	BID_PRICE
	Must be 0.00 or null


The Primary Transmission Provider shall evaluate each REDIRECT on a Non-Firm basis as any other non-firm point-to-point transmission service.  Provider business practices establish the requirements for service duration, submission time, evaluation time, confirmation time, etc.

OASIS or Transmission Provider procedures should verify that the transmission reservation identified in RELATED_REF meets all the requirements to support the redirect of transmission rights to the new service points.  This should include the validation that the current rights, the Capacity Available for Redirect, held on that reservation in the amount of the REDIRECT over time have not be encumbered by any other confirmed redirects, resales, schedules, etc.  This capacity validation may occur at any point in the request process, but shall always be performed at the time the REDIRECT STATUS is attempting to be set to CONFIRMED.

Once CONFIRMED, the transmission rights held on the RELATED_REF reservation in the amount of the REDIRECT shall be removed from the Capacity Available for Redirect on that reservation. Should the Customer wish to restore the rights to schedule (or redirect, resell, etc.) under the RELATED_REF reservation, they must submit a RELINQUISH request to the Primary Transmission Provider to release the capacity held under the REDIRECT request and reinstate that capacity on the original service  points. The Transmission Provider must accommodate this release of capacity back to the original service points, and shall through OASIS or Transmission Provider procedures insure that honoring this release of capacity and subsequent scheduling under the Customer’s original firm reservation will not unduly cause a reliability problem.
011-2.13
RELINQUISH Requests 

The RELINQUISH request is submitted by the Transmission Customer to indicate their desire to release transmission capacity rights held on an existing confirmed reservation.  The following are the recognized required uses for the RELINQUISH request that must be supported on OASIS.

	Use
	Description

	Redirect on Non-Firm Basis
	Releases capacity from a confirmed REDIRECT on a non-firm basis to the parent firm reservation


Note that the RELINQUISH request does not in itself represent a reservation for transmission service, but merely documents an action taken against an existing transmission service reservation. 

The specific requirements for the RELINQUISH request for each of these uses is detailed in the following Standards.

011-2.13.1
RELINQUISH of Redirect on a Non-Firm Basis
The RELINQUISH request in association with a REDIRECT request on a non-firm basis indicates the Customer’s desire to return the capacity rights held on the REDIRECT to the parent reservation specified in the RELATED_REF of that REDIRECT request.  The following are the specific requirements for the RELINQUISH request submitted via the transrequest template.

	Data Element
	Restriction/Requirement

	REQUEST_TYPE
	Must be RELINQUISH

	RELATED_REF
	Must specify the ASSIGNMENT_REF of a confirmed REDIRECT on a non-firm basis held by the Customer


	SELLER_CODE
	Must match PRIMARY_PROVIDER_CODE

	SELLER_DUNS
	Must match PRIMARY_PROVIDER_DUNS

	PATH
	Must represent the same corresponding service points in the reservation/request specified in RELATED_REF

	POINT_OF_RECEIPT
	

	POINT_OF_DELIVERY
	

	SOURCE
	

	SINK
	

	SERVICE_INCREMENT
	Must represent the same set of valid transmission service attributes specified in RELATED_REF

	TS_CLASS
	

	TS_TYPE
	

	TS_PERIOD
	

	TS_WINDOW
	

	TS_SUBCLASS
	

	START_TIME
	Must specify start of the interval for the release of capacity from RELATED_REF 

	STOP_TIME
	Must specify stop/end of the interval for the release of capacity from RELATED_REF

	CAPACITY_REQUESTED
	Must specify the capacity to be released from RELATED_REF over START_TIME to STOP_TIME interval and restored to the parent reservation (i.e., RELATED_REF’s RELATED_REF)

	BID_PRICE
	Must be 0.00 or null

	PRECONFIRMED
	Must be YES


When accepted by the Primary Transmission Provider, OASIS or Transmission Provider procedures must remove the capacity held on the REDIRECT request over the time interval specified, and reinstate that capacity to the Capacity Available for Redirect of the parent firm reservation.
011-2.14
RECALL Requests 

[ed. We need to decide if we want to allow Reseller’s the ability to undo RESALE transactions using this request.  If so, it should be a required OASIS request type.  If it is solely optional for TP to document cases of recalling capacity, it can remain optional as the reduction template requirements provide the necessary structures to report any reductions in capacity available on a reservation due to TP recalls.  I have written the following to require it to allow Resellers the ability to backout of RESALEs.
If we allow RECALL in the hands of Reseller’s, we need to extend the transassign template to add the REQUEST_TYPE and RELATED_REF data elements.  If we wanted to dictate some specific use/handling by the TP, we could consider adding SELLER_xxx and STATUS as possible extensions (unrelated to its use for RECALL).]
The RECALL request is submitted by the Seller to an existing confirmed reservation to document the recalling of capacity from that confirmed reservation for cause.  It is similar to RELINQUISH, a Customer’s voluntary release of capacity held on a reservation, but is a Seller’s unilateral taking back of capacity conveyed to the Customer by a preceding transaction.  As a Seller specific transaction requiring no Customer action, submission of RECALL requests is implemented through the transassign template. 
The following are the recognized uses for the RECALL request that should be supported on OASIS.

	Use
	Description

	Recall of resold capacity
	Recalls the capacity sold to an Assignee by the Reseller via a confirmed RESALE, and reinstates that capacity to the Reseller. Required.

	Recall by the Primary Transmission Provider
	Recalls the capacity held on any confirmed OASIS reservation by the Primary Transmission Provider for cause. Optional.


Note that the RECALL request does not in itself represent a reservation for transmission service, but merely documents an action taken against an existing transmission service reservation. 

The specific requirements for the RECALL request for each of these uses is detailed in the following Standards.

011-2.14.1
RECALL of Resold Capacity
The Reseller to a RESALE transaction may submit the RECALL request to recall capacity held on the RESALE reservation and reinstate that capacity on one or more of the Reseller’s reservations that supported the resale.

The following are the specific requirements for the RECALL request submitted via the transassign template.

	Data Element
	Restriction/Requirement

	REQUEST_TYPE
	Must be RECALL

	RELATED_REF
	Must specify the ASSIGNMENT_REF of a confirmed RESALE sold by the submitter to the Customer 


	CUSTOMER_CODE
	Must correspond with the Customer in the reservation specified in RELATED_REF

	CUSTOMER_DUNS
	Must correspond with the Customer in the reservation specified in RELATED_REF

	PATH
	Must represent the same corresponding service points in the reservation/request specified in RELATED_REF

	POINT_OF_RECEIPT
	

	POINT_OF_DELIVERY
	

	SOURCE
	

	SINK
	

	SERVICE_INCREMENT
	Must represent the same set of valid transmission service attributes specified in RELATED_REF

	TS_CLASS
	

	TS_TYPE
	

	TS_PERIOD
	

	TS_WINDOW
	

	TS_SUBCLASS
	

	START_TIME
	Must specify start of the interval for the recall of capacity from RELATED_REF 

	STOP_TIME
	Must specify stop/end of the interval for the recall of capacity from RELATED_REF

	CAPACITY_REQUESTED
	Must specify the total amount of capacity to be recalled from RELATED_REF over START_TIME to STOP_TIME interval and restored to the Reseller

	CAPACITY_GRANTED
	Must be identical to CAPACITY_REQUESTED

	OFFER_PRICE
	Must be 0.00 or null

	REASSIGNED_REF
	Collectively represent those confirmed transmission reservations held by the Reseller whose rights are to be reinstated in the amounts and over the times specified

	REASSIGNED_CAPACITY
	

	REASSIGNED_START_TIME
	

	REASSIGNED_STOP_TIME
	


When submitted by the Reseller to OASIS, OASIS or Transmission Provider procedures must verify all data elements and validate that each of the reservations specified by RELATED_REF are valid confirmed reservations held by the Reseller (submitter), and that the sum of capacity over time represented in the data elements REASSIGNED_CAPACITY, REASSIGNED_START_TIME and REASSIGNED_STOP_TIME exactly equals the total capacity being recalled from RELATED_REF as specified in CAPACITY_GRANTED, START_TIME and STOP_TIME.

If all validations are successful, OASIS or Transmission Provider procedures shall recall the capacity from the Assignee and reinstate that capacity to each of the Reseller’s reservations specified.  The recall of capacity shall be posted as a reduction against RELATED_REF.  The reinstatement of capacity to REASSIGNED_REF shall be posted as a credit, or positive adjustment to the existing reduction posted by confirmation of the RESALE.
011-2.14.2
RECALL by the Primary Transmission Provider

Use of a RECALL transaction by the Primary Transmission Provider to document circumstances where capacity has been recalled from a confirmed OASIS transmission reservation is optional.  The Primary Transmission Provider is required to document all such actions by posting information to OASIS viewable by the Customer using the reduction template.  If the RECALL transaction is used, it is in addition to the required reduction template postings.
If the Primary Transmission Provider elects to use the RECALL request, the following are the specific data requirements to be posted on OASIS for the RECALL.

	Data Element
	Restriction/Requirement

	REQUEST_TYPE
	Must be RECALL

	RELATED_REF
	Must specify the ASSIGNMENT_REF of a confirmed OASIS transmission service reservation (i.e., not RECALL or RELINQUISH).



	CUSTOMER_CODE
	Must correspond with the Customer in the reservation specified in RELATED_REF

	CUSTOMER_DUNS
	Must correspond with the Customer in the reservation specified in RELATED_REF

	PATH
	Must represent the same corresponding service points in the reservation/request specified in RELATED_REF

	POINT_OF_RECEIPT
	

	POINT_OF_DELIVERY
	

	SOURCE
	

	SINK
	

	SERVICE_INCREMENT
	Must represent the same set of valid transmission service attributes specified in RELATED_REF

	TS_CLASS
	

	TS_TYPE
	

	TS_PERIOD
	

	TS_WINDOW
	

	TS_SUBCLASS
	

	START_TIME
	Must specify start of the interval for the recall of capacity from RELATED_REF 

	STOP_TIME
	Must specify stop/end of the interval for the recall of capacity from RELATED_REF

	CAPACITY_REQUESTED
	Must specify the total amount of capacity to be recalled from RELATED_REF over START_TIME to STOP_TIME interval and restored to the Reseller

	CAPACITY_GRANTED
	Must be identical to CAPACITY_REQUESTED


When posted on OASIS, OASIS or Transmission Provider procedures shall recall the capacity from the RELATED_REF and be posted as a reduction against RELATED_REF.  Capacity recalled by the Primary Transmission Provider is reinstated to the Provider’s  Available Transfer Capability (ATC/AFC).
011-3
SPECIFIC TEMPLATE IMPLEMENTATION
[ed: Need to discuss if there are specific OASIS templates whose implementation has been subject to different interpretations.  Scheduledetail may be one example.]

011-4
FILE REQUEST AND FILE DOWNLOAD EXAMPLES

In the examples, the end-of-line (eol) character is represented by the character," ( ". This symbol may appear different on displays or printouts.

011-4.1
File Example for Hourly Offering

Example of the request to Primary Provider, aaa, and response for Seller, wxyz, for PATH_NAME "W/AAAA/PATH-ABC//" for April 10, 1996 from 8 a.m. to 3 p.m. (Note that the PATH_NAME consists of a REGION_CODE, PRIMARY_PROVIDER_CODE, PATH_CODE, and an OPTIONAL_CODE, separated with a slash, "/".) 
The VERSION for this release is 1.4. The request is in the form of a URL query string and the response is an ASCII delimited file.

1. Query

http://(OASIS Node name)/OASIS/aaa/data/transoffering? ver=1.2&templ=transoffering& fmt=data&pprov=AAAA &pprovduns=123456789& path=W/AAA/ABC// &seller=WXYZAA &sellerduns=987654321& POR=aaa& POD=bbb& servincre=hourly& TSCLASS1=firm &TSCLASS2=non-firm&tz=PD&stime=19960410080000PD&sptime= 19960410150000PD

2. Response Data

REQUEST-STATUS=200( (Successful)

TIME_STAMP=19960409113526PD (
VERSION=1.4(
TEMPLATE=transoffering(
OUTPUT_FORMAT=DATA (
PRIMARY_PROVIDER_CODE=AAAA(
PRIMARY_PROVIDER_DUNS=123456789(
DATA_ROWS=14(
COLUMN_HEADERS=TIME_OF_LAST_UPDATE,SELLER_CODE,SELLER_DUNS,PATH_NAME,

POINT_OF_RECEIPT,POINT_OF_DELIVERY,INTERFACE_TYPE,OFFER_START_TIME, OFFER_STOP_TIME,

START_TIME,STOP_TIME, CAPACITY, SERVICE_INCREMENT, TS_CLASS, TS_TYPE, TS_PERIOD,

TS_SUBCLASS, SALE_REF, POSTING_REF, CEILING_PRICE, OFFER_PRICE, PRICE_UNITS,

SERVICE_DESCRIPTION,SELLER_NAME,SELLER_PHONE,SELLER_FAX, SELLEREMAIL,

SELLER_COMMENTS (
19960409030000PD,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,19960402080000PD,19960410080000PD,19960410

080000PD,19960410090000PD,300, HOURLY, FIRM, POINT_TO_POINT, OFF_PEAK, N/A, N/A, A001,

1.50,1.35,MW,N/A,N/A,N/A,N/A,N/A,10% DISCOUNT (
19960409030000PD,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,19960402080000PD,19960410080000PD,19960410

080000PD,19960410090000PD,300, HOURLY, NON-FIRM, POINT_TO_POINT, OFF_PEAK, N/A, N/A,A001,1.50,

1.35,MW,N/A,N/A,N/A,N/A,N/A, 10% DISCOUNT (
19960409030000PD,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,19960402080000PD,19960410080000PD,19960410

090000PD,1996041010000PD,300, HOURLY, FIRM, POINT_TO_POINT, OFF_PEAK, N/A,

N/A,A001,1.50,1.35,MW,N/A,N/A,N/A,N/A,N/A,10% DISCOUNT (
19960409030000PD,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,19960402080000PD,19960410080000PD,19960410

090000PD,19960410100000PD,300, HOURLY, NON-FIRM, POINT_TO_POINT, OFF_PEAK, N/A, N/A,A001,1.50,

1.35,MW,N/A,N/A,N/A,N/A,N/A, 10% DISCOUNT (
19960409030000PD,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,19960402080000PD,19960410080000PD,19960410

100000PD,19960410110000PD,300, HOURLY, FIRM, POINT_TO_POINT, OFF_PEAK, N/A,

N/A,A001,1.50,1.35,MW,N/A,N/A,N/A,N/A,N/A,10% DISCOUNT (
19960409030000PD,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,19960402080000PD,19960410080000PD,19960410

100000PD,19960410110000PD,300, HOURLY, NON-FIRM, POINT_TO_POINT, OFF_PEAK, N/A, N/A,A001,1.50,

1.35,MW,N/A,N/A,N/A,N/A,N/A, 10% DISCOUNT (
19960409030000PD,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,19960402080000PD,19960410080000PD,19960410

110000PD,19960410120000PD,300, HOURLY, FIRM, POINT_TO_POINT, OFF_PEAK, N/A,

N/A,A001,1.50,1.35,MW,N/A,N/A,N/A,N/A,N/A,10% DISCOUNT (
19960409030000PD,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,19960402080000PD,19960410080000PD,19960410

110000PD,19960410120000PD,300, HOURLY, NON-FIRM, POINT_TO_POINT, OFF_PEAK, N/A, N/A,A001,1.50,

1.35,MW,N/A,N/A,N/A,N/A,N/A, 10% DISCOUNT (
. . .

. . .

. . .

19960409030000PD,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,19960402080000PD,19960410080000PD,19960410

140000PD,19960410150000PD,300, HOURLY, FIRM, POINT_TO_POINT, OFF_PEAK, N/A,

N/A,A001,1.50,1.35,MW,N/A,N/A,N/A,N/A,N/A,10% DISCOUNT (
19960409030000PD,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,19960402080000PD,19960410080000PD,19960410

140000PD,19960410150000PD,300, HOURLY, NON-FIRM, POINT_TO_POINT, OFF_PEAK, N/A, N/A,A001,1.50,

1.35,MW,N/A,N/A,N/A,N/A,N/A, 10% DISCOUNT (
011-4.2
File Example for Hourly Schedule Data

This example shows a request for the hourly schedule data from Primary Provider, AAAA, related to the seller, WXYZ, for the period 10 a.m. to 3 p.m. on April 10, 2000. 
There are two identical requests examples using two slightly different methods. The first request is using a HTTP URL request string through an HTML GET method. The second request is a similar example using fetch_http from a file using a POST method.

1. Query

URL Request (HTTP method=GET) 
http://(OASIS Node name)/OASIS/aaaa/data/scheduledetail? ver=1.4& pprov=AAAA& templ=scheduledetail& fmt=data &pprovduns=123456789 &path=W/AAA/ABC//& seller=WXYZ &por=BBB &pod=CCC& tz=PD& stime=20000410100000PD& sptime=20000410150000PD

URL Request (HTTP method=POST) 
$ fetch_http http://(OASIS Node name)/OASIS/aaaa/data/OASISdata -f c:/OASIS/wxyz/upload/infile. txt Where in-file.txt contains the following: ver=1.4& pprov=AAAA& templ=scheduledetail& fmt=data &pprovduns=123456789 &path=W/AAA/ABC//& seller=WXYZ &por=BBB &pod=CCC& tz=PD& stime=20000410100000PD& sptime=20000410150000PD

2. Response Data

REQUEST_STATUS=200(
ERROR_MESSAGE=No error. (
TIME_STAMP=20000410160523ES(
VERSION=1.4(
TEMPLATE=scheduledetail(
OUTPUT_FORMAT=DATA(
PRIMARY_PROVIDER_CODE=AAAA(
PRIMARY_PROVIDER_DUNS=123456789(
RETURN_TZ=PD(
DATA_ROWS=3(
COLUMN_HEADERS=CONTINUATION_FLAG, TIME_OF_LAST_UPDATE, SCHEDULE_REF, TRANSACTION_ID, PATH_NAME, POINT_OF_RECEIPT, POINT_OF_DELIVERY, GCA_CODE, LCA_CODE, SOURCE, SINK, SCHEDULE_PRIORITY, START_TIME, STOP_TIME, SCHEDULE_REQUESTED, SCHEDULE_GRANTED, ASSIGNMENT_REF, SELLER_CODE, SELLER_DUNS, CUSTOMER_CODE, CUSTOMER_DUNS, AFFILIATE_FLAG, SERVICE_INCREMENT, TS_CLASS, TS_TYPE, TS_PERIOD, TS_WINDOW, TS_SUBCLASS, NERC_CURTAILMENT_PRIORITY, OTHER_CURTAILMENT_PRIORITY, CAPACITY_USED, PROVIDER_ACTION, SCHEDULE_LIMIT, CURTAILMENT_OPTIONS, SECURITY_REF, INITIATING_PARTY, RESPONSIBLE_PARTY, PROCEDURE_NAME, PROCEDURE_LEVEL, FACILITY_LOCATION, FACILITY_NAME, FACILITY_CLASS, FACILITY_LIMIT_TYPE(
N, 20000409030000PD,12345,2233, W/AAA/ABC//, BBB, CCC,,,,,1, 20000410100000PD, 20000410110000PD,300,300,856743, wxyz,987654321, WXYZAA,987654322, Y, HOURLY, NON_FIRM, POINT_TO_POINT, OFF_PEAK, FIXED,,1,1,300,,,,,,,,,,,, (
N, 20000409030000PD,12346,2233, W/AAA/ABC//, BBB, CCC,,,,,1, 20000410130000PD, 20000410140000PD,300,300,856743,wxyz,987654321, WXYZAA,987654322, Y, HOURLY, NON_FIRM, POINT_TO_POINT, OFF_PEAK, FIXED,,1,1,300,,,,,,,,,,,, (
N, 20000409030000PD,12347,2233, W/AAA/ABC//, BBB, CCC,,,,,1, 20000410140000PD, 20000410150000PD,300,300,856743,wxyz,987654321, WXYZAA,987654322, Y, HOURLY, NON_FIRM, POINT_TO_POINT, OFF_PEAK, FIXED,,1,1,300,,,,,,,,,,,, (
011-4.3
Customer Posting a Transmission Service Offering

This example shows how a Customer would post for sale the transmission service that was purchased previously. The Seller would create a file and upload the file using the FETCH_HTTP program to send a file to the OASIS Node of the Primary Provider.

1. Input:

VERSION=1.4(
TEMPLATE=transpost(
OUTPUT_FORMAT=DATA (
PRIMARY_PROVIDER_CODE=AAAA(
PRIMARY_PROVIDER_DUNS=123456789(
DATA_ROWS=1(
COLUMN_HEADERS=PATH_NAME, POINT_OF_RECEIPT, POINT_OF_DELIVERY, INTERFACE_TYPE, CAPACITY, SERVICE_INCREMENT, TS_CLASS, TS_TYPE, TS_PERIOD, TS_SUBCLASS, START_TIME, STOP_TIME, OFFER_START_TIME, OFFER_STOP_TIME, SALE_REF, OFFER_PRICE, SERVICE_DESCRIPTION, SELLER_COMMENTPF(
 WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,150, HOURLY, FIRM, POINT_TO_POINT, OFF_PEAK, N/A,, 19960402080000PD,19960410080000PD, 19960410080000PD,19960410150000PD, A123,.90,N/A,"As Joe said, ""It is a good buy"""(
FETCH_HTTP Command to send posting $ fetch_http http://(OASIS Node name)/OASIS/abcd/data/transrequest -f c:/OASIS/abcd/upload/post.txt

2. Response Data

REQUEST-STATUS=200 ( (Successful)

TIME_STAMP=19960409113526PD (
VERSION=1.4(
TEMPLATE=transpost(
OUTPUT_FORMAT=DATA (
PRIMARY_PROVIDER_CODE=AAAA(
PRIMARY_PROVIDER_DUNS=123456789(
DATA_ROWS=1(
COLUMN_HEADERS=RECORD_STATUS, PATH_NAME, POINT_OF_RECEIPT, POINT_OF_DELIVERY, INTERFACE_TYPE, CAPACITY, SERVICE_INCREMENT, TS_CLASS, TS_TYPE, TS_PERIOD, TS_SUBCLASS, START_TIME, STOP_TIME, OFFER_START_TIME, OFFER_STOP_TIME, SALE_REF, OFFER_PRICE, SERVICE_DESCRIPTION, SELLER_COMMENTS, ERROR_MESSAGE(
200,WXYZ,987654321,W/AAA/ABC//,N/A,N/A,E,150, HOURLY, FIRM, POINT_TO_POINT, OFF_PEAK, N/A, 19960402080000PD,19960410080000PD, 19960410080000PD,19960410150000PD, A123,.90,N/A, "As Joe said, ""It is a good buy""", No Error(
011-4.4
Example of Re-aggregating Purchasing Services using Reassignment

The following examples do not show the complete Template information, but only show those elements of the Template of interest to the example.

a. Customer #1, "BestE" requests the purchase of 150 MW Firm ATC for 8 a.m. to 5 p.m. for $1.00 from a Primary Provider (transrequest).

TEMPLATE=transrequest(
CUSTOMER_CODE=BestE(
CAPACITY=150(
TS_CLASS="FIRM"(
START_TIME="1996050708000000PD"(
STOP_TIME="1996050717000000PD"(
BID_PRICE="$1.00"(
The Information Provider assigns ASSIGNMENT_REF = 5000 on acknowledgment.

b. Customer #1 purchases 120 MW ATC Non-firm for 3 p.m. to 9 p.m. for $.90 (transrequest). The Information Provider assigns the ASSIGNMENT_REF=5001 when the request for purchase is made and is shown in the acknowledgment.

TEMPLATE="transrequest"(
CUSTOMER_CODE="BestE"(
CAPACITY=120(
TS_CLASS="NON-FIRM"(
START_TIME="1996050715000000PD"(
STOP_TIME="1996050721000000PD"(
BID_PRICE="$1.05"(
c. Customer #1 becomes Seller #1 and post the Transmission service of 100 MW ATC Non-firm capacity from 8 a.m. to 9 p.m. for resale at $.90/MW-hour.

TEMPLATE="transpost"(
SELLER_CODE="BestE"(
CAPACITY=100(
TS_CLASS="NON-FIRM"(
START_TIME="1996050708000000PD"(
STOP_TIME="1996050721000000PD"(
SALE_REF="BEST100"(
OFFER_PRICE=.90(
SELLER_COMMENTS="aggregating two previous purchases"(
d. Customer #2 then requests purchase of 100 MW Non-firm from Reseller #1 from 8 a.m. to 6 p.m. for $0.90/MW-hour (transrequest).

TEMPLATE="transrequest"(
CUSTOMER_CODE="Whlsle"(
SELLER_CODE="BestE"(
CAPACITY=100(
TS_CLASS="NON-FIRM"(
START_TIME="1996050708000000PD"(
STOP_TIME="1996050721000000PD"(
SALE_REF="BEST100"(
DEAL_REF="WPC100"(
BID_PRICE=.90(
CUSTOMER_COMMENTS="Only need service until 6 p.m." (
The Information Provider provides the ASSIGNMENT_REF=5002 for this transaction.

e. Seller informs the Information Provider of the reassignment of the previous transmission rights when the seller accepts the customer purchase request (transsell).

TEMPLATE="transsell"(
CUSTOMER_CODE="Whlsle"(
SELLER_CODE="BestE"(
ASSIGNMENT_REF=5002(
STATUS="Accepted"(
REASSIGNED_REF1=5000(
REASSIGNED_CAPACITY1=100(
REASSIGNED_START_TIME1="199605070800PD"(
REASSIGNED_STOP_TIME1="199605071700PD"(
REASSIGNED_REF2=5001(
REASSIGNED_CAPACITY2=100(
REASSIGNED_START_TIME2="199605071700PD"(
REASSIGNED_STOP_TIME2="199605071800PD"(
011-4.5
File Examples of the Use of Continuation Records

a. Basic Continuation Records

The first example of the use of Continuation Records is for the transrequest Template submitted by a Seller for purchase of a transmission reservation spanning 16 hours from 06:00 to 22:00 with "ramped" demand at beginning and end of time period. Two additional reservations appear prior to and following the profile to demonstrate the handling of ASSIGNMENT_REF by the OASIS Node.
Only the following fields may be redefined in a continuation record for the transrequest   Template: CAPACITY_GRANTED, START_TIME, STOP_TIME. Specification of any values corresponding to COLUMN_HEADERs other than CAPACITY-GRANTED, START_TIME, and STOP_TIME will be ignored, however commas must be included to properly align the CAPACITY_GRANTED, START_TIME and STOP_TIME fields.

Input:

VERSION=1.4(
TEMPLATE=transrequest(
OUTPUT_FORMAT=DATA(
PRIMARY_PROVIDER_CODE=AEP(
PRIMARY_PROVIDER_DUNS=123456789(
RETURN_TZ=ES(
DATA_ROWS=7(
COLUMN_HEADERS=CONTINUTATION_FLAG, SELLER_CODE,SELLER_DUNS, PATH_NAME, POINT_OF_RECEIPT, POINT_OF_DELIVERY, SOURCE, SINK,CAPACITY_REQUESTED, SERVICE_INCREMENT, TS_CLASS, TS_TYPE, TS_PERIOD, TS_WINDOW, TS_SUBCLASS, STATUS_NOTIFICATION,START_TIME,STOP_TIME,BID_PRICE, PRECONFIRMED, ANC_SVC_LNK, POSTING_REF, SALE_REF, REQUEST_REF, DEAL_REF, CUSTOMER_COMMENTS, REQUEST_TYPE,REASSIGNED_REF(
N, AEP,123456789, ABC/XY, CE, MECS,,,35, DAILY, FIRM, POINT_TO_POINT, FULL_PERIOD, FIXED,, pub/AEP/incoming,20000423000000ES,20000424000000ES,24.5, Y, SC:(AEP:RQ);RV:(AEP:RQ);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, P0123 , S123, R765, D123, Standard daily reservation, ORIGINAL, (
N, AEP,123456789, ABC/XY, CE, AMPO,,,5, HOURLY, NON-FIRM, POINT_TO_POINT, FULL_PERIOD, FIXED,, pub/AEP/incoming,20000423060000ES,20000423070000ES,2.5, Y, SC:(AEP:RQ);RV:(AEP:RQ);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, P0123 , S123, R765, D123, First piece of profile spanning 5 records, ORIGINAL, (
Y,,,,,,,,10,,,,,,, ,20000423070000ES,20000423080000ES,,,,,,,, Second piece,, (
Y,,,,,,,,15,,,,,,, ,20000423080000ES,20000423200000ES,,,,,,,, Third piece,, (
Y,,,,,,,,10,,,,,,, ,20000423200000ES,20000423210000ES,,,,,,,, Fourth piece,, (
Y,,,,,,,,5,,,,,,, ,20000423210000ES,20000423220000ES,,,,,,,, Fifth piece,, (
N, AEP,123456789, ABC/XY, CE, MECS, , ,20, HOURLY, NON-FIRM, POINT_TO_POINT, FULL_PERIOD, FIXED,, pub/AEP/incoming,20000423040000ES,20000423160000ES,2, Y, SC:(AEP:RQ);RV:(AEP:RQ);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, P0123 , S123, R765, D123, Standard hourly reservation after profiled reservation, ORIGINAL, (
Response:

REQUEST_STATUS=200(
ERROR_MESSAGE=Successfully updated. (
TIME_STAMP=20000422160523ES(
VERSION=1.4(
TEMPLATE=transrequest(
OUTPUT_FORMAT=DATA(
PRIMARY_PROVIDER_CODE=AEP(
PRIMARY_PROVIDER_DUNS=123456789(
RETURN_TZ=ES(
DATA_ROWS=7(
COLUMN_HEADERS=RECORD_STATUS, CONTINUTATION_FLAG, ASSIGNMENT_REF, SELLER_CODE,SELLER_DUNS, PATH_NAME, POINT_OF_RECEIPT, POINT_OF_DELIVERY, SOURCE, SINK,CAPACITY_REQUESTED, SERVICE_INCREMENT, TS_CLASS, TS_TYPE, TS_PERIOD, TS_WINDOW, TS_SUBCLASS, STATUS_NOTIFICATION,START_TIME,STOP_TIME,BID_PRICE, PRECONFIRMED, ANC_SVC_LNK, POSTING_REF, SALE_REF, REQUEST_REF, DEAL_REF, CUSTOMER_COMMENTS, REQUEST_TYPE,REASSIGNED_REF, ERROR_MESSAGE(
200,N,8234, AEP,123456789, ABC/XY, CE, MECS,,,35, DAILY, FIRM, POINT_TO_POINT, FULL_PERIOD, FIXED,, pub/AEP/incoming,20000423000000ES,20000424000000ES,24.5, Y, SC:(AEP:RQ);RV:(AEP:RQ);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, P0123 , S123, R765, D123, Standard daily reservation, ORIGINAL,, No error(
200,N,8235, AEP,123456789, ABC/XY, CE, AMPO,,,5, HOURLY, NON-FIRM, POINT_TO_POINT, FULL_PERIOD, FIXED,, pub/AEP/incoming,20000423060000ES,20000423070000ES,2.5, Y, SC:(AEP:RQ);RV:(AEP:RQ);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, P0123 , S123, R765, D123, First piece of profile spanning 5 records, ORIGINAL,, No error(
200,Y,8235,,,,,,,,10,,,,,,,,20000423070000ES,20000423080000ES,,,,,,,, Second piece,,, No error(
200,Y,8235,,,,,,,,15,,,,,,,,20000423080000ES,20000423200000ES,,,,,,,, Third piece,,, No error(
200,Y,8235,,,,,,,,10,,,,,,,,20000423200000ES,20000423210000ES,,,,,,,, Fourth piece,,, No error(
200,Y,8235,,,,,,,,5,,,,,,,,20000423210000ES,20000423220000ES,,,,,,,, Fifth piece,,, No error(
200,N,8236, AEP,123456789, ABC/XY, CE, MECS,,,20, HOURLY, NON-FIRM, POINT_TO_POINT, FULL_PERIOD, FIXED,, pub/AEP/incoming,20000423040000ES,20000423160000ES,2, Y, SC:(AEP:RQ);RV:(AEP:RQ);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, P0123 , S123, R765, D123, Standard hourly reservation after profiled reservation, ORIGINAL,, No error(
b. Submission of Reassignment Information - Case 1:

In the prior example, a reservation request was submitted to "Rseler" for 20MW of Hourly Non-firm service from 04:00 to 16:00. Assume that Rseler has previously reserved service for the CE-VP path for Daily Firm in amount of 50 MW on 4/23 under ASSIGNMENT_REF=7019, and Hourly Non-Firm in amount of 10 MW from 08:00 to 20:00 on 4/23 under ASSIGNMENT_REF=7880. Rseler must designate which transmission service rights are to be reassigned to Cust to satisfy the 20MW from 04:00 to 16:00. This reassignment information is conveyed by Rseler using the transsell Template when the reservation request is ACCEPTED. At the SELLER's discretion, rights are assigned from the Non-firm reservation first (ASSIGNMENT_REF=7880) with the balance taken up by the Firm reservation (ASSIGNMENT_REF=7019).

The only fields allowed in "continuation" records for transsell Template are REASSIGNED_REF, REASSIGNED_CAPACITY, REASSIGNED_START_TIME, and REASSIGNED_STOP_TIME. Price may not be negotiated for each "segment" in a capacity profile.

Input:

VERSION=1.4(
TEMPLATE=transsell(
OUTPUT_FORMAT=DATA(
PRIMARY_PROVIDER_CODE=AEP(
PRIMARY_PROVIDER_DUNS=123456789(
RETURN_TZ=ES(
DATA_ROWS=3(
COLUMN_HEADERS=CONTINUATION_FLAG,ASSIGNMENT_REF, START_TIME, STOP_TIME,OFFER_PRICE,CAPACITY_GRANTED, STATUS, STATUS_COMMENTS, ANC_SVC_LINK, ANC_SVC_REQ, NEGOTIATED_PRICE_FLAG, SELLER_REF, SELLER_COMMENTS, RESPONSE_TIME_LIMIT,REASSIGNED_REF,REASSIGNED_CAPACITY, REASSIGNED_START_TIME , REASSIGNED_STOP_TIME(
N,8236, 20000423040000ES, 20000423160000ES,2.5,20, ACCEPTED, Status comments here, SC:(AEP:RQ);RV:(AEP:RQ);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, SC:M;RV:M;RF:U;EI:U;SP:U;SU:U;,, S123, Seller comments here,,7019,20, 20000423040000ES, 20000423080000ES(
Y,8236,,, ,, , , ,,,, ,,7880,10, 20000423080000ES, 20000423160000ES(
Y,8236,,, ,, , , ,,,, ,,7019,10, 20000423080000ES, 20000423160000ES(
Response:

REQUEST_STATUS=200(
ERROR_MESSAGE=Successfully updated. (
TIME_STAMP=20000422160523ES(
VERSION=1.4(
TEMPLATE=transsell(
OUTPUT_FORMAT=DATA(
PRIMARY_PROVIDER_CODE=AEP(
PRIMARY_PROVIDER_DUNS=123456789(
RETURN_TZ=ES(
DATA_ROWS=3(
COLUMN_HEADERS=RECORD_STATUS,CONTINUATION_FLAG,ASSIGNMENT_REF, START_TIME, STOP_TIME,OFFER_PRICE,CAPACITY_GRANTED, STATUS, STATUS_COMMENTS, ANC_SVC_LINK, ANC_SVC_REQ, NEGOTIATED_PRICE_FLAG, SELLER_REF, SELLER_COMMENTS, RESPONSE_TIME_LIMIT,REASSIGNED_REF,REASSIGNED_CAPACITY, REASSIGNED_START_TIME , REASSIGNED_STOP_TIME, ERROR_MESSAGE(
N,,8236, 20000423040000ES, 20000423160000ES,2.5,20, ACCEPTED, Status comments here, SC:(AEP:RQ);RV:(AEP:RQ);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, SC:M;RV:M;RF:U;EI:U;SP:U;SU:U;,, S123, Seller comments here,,7019,20, 20000423040000ES, 20000423080000ES, No error(
Y,,8236,,, ,, , , ,,,, ,,7880,10, 20000423080000ES, 20000423160000ES, No error(
Y,,8236,,, ,, , , ,,,, ,,7019,10, 20000423080000ES, 20000423160000ES, No error(
c. Submission of Reassignment Information - Case 2:

Primary provider, AEP, is notified of a sale/assignment of transmission service rights from "Resell" to "cust". The parameters of the new reservation are for 10MW on 4/23 for "off-peak" hours (00:00- 06:00 and 22:00-24:00) on POR/POD CE-VP. Rseler is assigning rights to 10MW from a prior reservation for the CE-VP path for Daily Firm in amount of 50 MW on 4/23 under ASSIGNMENT_REF=7019 to Cust. AEP would submit the following information using the transassign Template to post this (re)sale. The only fields allowed in "continuation" records for the transassign Template are CAPACITY, START_TIME , STOP_TIME, REASSIGNED_REF, REASSIGNED_CAPACITY, REASSIGNED_START_TIME, and REASSIGNED_STOP_TIME. Even though there is a one-to-one correspondence between the segments of the new reservations and the reassignment of service from a prior reservation, it is entirely possible that a reservation spanning a single contiguous period would require multiple continuation records to convey reassignment information, and vice versa.
Fields for CUSTOMER_NAME and SELLER_NAME were used to convey user names for subsequent resolution of contact information from user registration.

Input:

VERSION=1.4(
TEMPLATE=transassign(
OUTPUT_FORMAT=DATA(
PRIMARY_PROVIDER_CODE=AEP(
PRIMARY_PROVIDER_DUNS=123456789(
RETURN_TZ=ES(
DATA_ROWS=2(
COLUMN_HEADERS=CONTINUATION_FLAG, CUSTOMER_CODE, CUSTOMER_DUNS, PATH_NAME, POINT_OF_RECEIPT, POINT_OF_DELIVERY, SOURCE, SINK, CAPACITY_REQUESTED, CAPACITY_GRANTED, SERVICE_INCREMENT, TS_CLASS, TS_TYPE, TS_PERIOD,TS_WINDOW, TS_SUBCLASS, START_TIME, STOP_TIME, OFFER_PRICE, ANC_SVC_LNK, POSTING_NAME, REASSIGNED_REF, REASSIGNED_CAPACITY, REASSIGNED_START_TIME , REASSIGNED_STOP_TIME , SELLER_COMMENTS, SELLER_REF(
N, ACSTMR,987654321, , CE, VP,,,10,10, HOURLY, NON-FIRM, POINT_TO_POINT, OFF_PEAK,FIXED,, 20000423000000ES, 20000423060000ES,2, SC:(AEP:RQ);RV:(AEP:RQ);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, Jane Doe ,7019,10, 20000423000000ES, 20000423060000ES, Seller comments go here, S123(
Y,,,,,,,,10,10,,,,,,, 20000423220000ES, 20000424000000ES,,,,7019,10, 20000423220000ES, 20000424000000ES,, (
Response:

REQUEST_STATUS=200(
ERROR_MESSAGE=Successfully updated. (
TIME_STAMP=20000422160523ES(
VERSION=1.4(
TEMPLATE=transassign(
OUTPUT_FORMAT=DATA(
PRIMARY_PROVIDER_CODE=AEP(
PRIMARY_PROVIDER_DUNS=123456789(
RETURN_TZ=ES(
DATA_ROWS=2(
COLUMN_HEADERS=RECORD_STATUS,CONTINUATION_FLAG,ASSIGNMENT_REF, CUSTOMER_CODE, CUSTOMER_DUNS, PATH_NAME, POINT_OF_RECEIPT, POINT_OF_DELIVERY, SOURCE, SINK, CAPACITY_REQUESTED, CAPACITY_GRANTED, SERVICE_INCREMENT, TS_CLASS, TS_TYPE, TS_PERIOD,TS_WINDOW, TS_SUBCLASS, START_TIME, STOP_TIME, OFFER_PRICE, ANC_SVC_LNK, POSTING_NAME, REASSIGNED_REF, REASSIGNED_CAPACITY, REASSIGNED_START_TIME , REASSIGNED_STOP_TIME , SELLER_COMMENTS, SELLER_REF5, ERROR_MESSAGE(
200,N,8207, ACSTMR,987654321, , CE, VP,,,10,10, HOURLY, NON-FIRM, POINT_TO_POINT, OFF_PEAK,FIXED,, 20000423000000ES, 20000423060000ES,2, SC:(AEP:RQ);RV:(AEP:RQ);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, Jane Doe ,7019,10, 20000423000000ES, 20000423060000ES, Seller comments go here, S1235, No error(
200,Y,8207,,,,,,,,10,10,,,,,,, 20000423220000ES, 20000424000000ES,,,,7019,10, 20000423220000ES, 20000424000000ES,,5, No error(
d. Query of Transmission Reservation Status:

The following typical response to a transstatus query might be delivered for 4/23 based on prior examples. Note that the only fields returned in "continuation" records are, ASSIGNMENT_REF, CAPACITY_REQUESTED, CAPACITY_GRANTED, START_TIME, STOP_TIME, REASSIGNED_REF, REASSIGNED_CAPACITY, REASSIGNED_START_TIME, and REASSIGNED_STOP_TIME (price fields are debatable).

Input:

<appropriate query name/value pairs to return reservations for 4/23>

Response:

REQUEST_STATUS=200(
ERROR_MESSAGE=No error. (
TIME_STAMP=20000423160523ES(
VERSION=1.4(
TEMPLATE=transstatus(
OUTPUT_FORMAT=DATA(
PRIMARY_PROVIDER_CODE=AEP(
PRIMARY_PROVIDER_DUNS=123456789(
RETURN_TZ=ES(
DATA_ROWS=11(
COLUMN_HEADERS=CONTINUATION_FLAG, ASSIGNMENT_REF, SELLER_CODE, SELLER_DUNS, CUSTOMER_CODE, CUSTOMER_DUNS, AFFILIATE_FLAG, PATH_NAME, POINT_OF_RECEIPT, POINT_OF_DELIVERY, SOURCE, SINK, CAPACITY_REQUESTED, CAPACITY_GRANTED, SERVICE_INCREMENT, TS_CLASS, TS_TYPE, TS_PERIOD,TS_WINDOW, TS_SUBCLASS, NERC_CURTAILMENT_PRIORITY, OTHER_CURTAILMENT_PRIORITY, START_TIME , STOP_TIME, CEILING_PRICE, OFFER_PRICE, BID_PRICE,PRICE_UNITS, PRECONFIRMED, ANC_SVC_LINK, ANC_SVC_REQ, POSTING_REF, SALE_REF, REQUEST_REF, DEAL_REF,IMPACTED,REQUEST_TYPE,RELATED_REF, NEGOTIATED_PRICE_FLAG, STATUS,STATUS_NOTIFICATION, STATUS_COMMENTS, TIME_QUEUED, TIME_OF_LAST_UPDATE, PRIMARY_PROVIDER_COMMENTS,SELLER_REF, SELLER_COMMENTS, CUSTOMER_COMMENTS, SELLER_NAME, SELLER_PHONE, SELLER_FAX, SELLER_EMAIL, CUSTOMER_NAME, CUSTOMER_PHONE, CUSTOMER_FAX, CUSTOMER_EMAIL, REASSIGNED_REF, REASSIGNED_CAPACITY, REASSIGNED_START_TIME , REASSIGNED_STOP_TIME(
N,8207, RSELLR,234567890, ACSTMR,987654321, N, , CE, VP, ,,10,10, HOURLY, FIRM, POINT_TO_POINT, OFF_PEAK,,,,, 20000423000000ES, 20000423060000ES,2.25,2,2,$/MW, N, SC:(AEP:AR:121);RV:(AEP:AR:122);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, SC:M;RV:M;RF:U;EI:U;SP:U;SU:U;, ,S1235, , ,0, RESALE,, L, CONFIRMED,, , 20000422121354ES, 20000422123054ES, TP Comments,, Seller comments go here, Customer comments, Joe Smith, (888)-123-4567, (888)-123-1231, jsmith@xyz.com, Jane Doe, (999)-123-4567, (999)-123-8823,,7019,10, 20000423000000ES, 20000423060000ES(
Y,8207,,,,,,,,,,,10,10,,,,,,,,, 20000423220000ES, 20000424000000ES,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,7019,10, 20000423220000ES, 20000424000000ES(
N,8234, AEP,123456789, CUSTMR,345678912, N, , CE, MECS, ,,35,35, DAILY, FIRM, POINT_TO_POINT,FULL_PERIOD,FIXED,,,, 20000423000000ES, 20000423060000ES,42,24.5,24.5,$/MW, N, SC:(AEP:AR:123);RV:(AEP:AR:124);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, SC:M;RV:M;RF:U;EI:U;SP:U;SU:U;, P0123 , S123, R765, D123,0, ORIGINAL,, L, CONFIRMED, pub/AEP/incoming,, 20000422131354ES, 20000422133354ES, Standard daily reservation,, System Operator, Customer comments, Frank Orth, (999)-123-4567, (999)-123-1231, jsmith@xyz.com, Jane Doe, (999)-123-4567, (999)-123-8823,,7019,10, 20000423000000ES, 20000423060000ES(
N,8235, AEP,123456789, CUSTMR,345678912, N, , CE, AMPO, ,,5,5, HOURLY, NON-FIRM, POINT_TO_POINT,FULL_PERIOD,FIXED,,,, 20000423060000ES, 20000423070000ES,2.5,2.5,2.5,$/MW, N, SC:(AEP:AR:125);RV:(AEP:AR:126);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, SC:M;RV:M;RF:U;EI:U;SP:U;SU:U;, P0123 , S123, R765, D123,0, ORIGINAL,,, CONFIRMED, pub/AEP/incoming,, 20000422160523ES, 20000422170523ES, Profile verified,, First piece, Customer comments, System Operator, (888)-123-4567, (888)-123-1231, jsmith@xyz.com, Jane Doe, (999)- 123-4567, (999)-123-8823,,7019,10, 20000423000000ES, 20000423060000ES(
Y,8235,,,,,,,,,,,10,10,,,,,,,,, 20000423070000ES, 20000423080000ES,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,5 Y,8235,,,,,,,,,,,15,15,,,,,,,,, 20000423080000ES, 20000423200000ES,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,, (
Y,8235,,,,,,,,,,,10,10,,,,,,,,, 20000423200000ES, 20000423210000ES,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,5 Y,8235,,,,,,,,,,,5,5,,,,,,,,, 20000423210000ES, 20000423220000ES,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,, (
N,8236, AEP,123456789, CUSTMR,345678912, N, , CE, VP, ,,20,20, HOURLY,NON_FIRM, POINT_TO_POINT,FULL_PERIOD,FIXED,,,, 20000424040000ES, 20000424160000ES,2.5,2.5,2.5,$/MW, N, SC:(AEP:AR:127);RV:(AEP:AR:128);RF:(FT);EI:(FT);SP:(FT);SU:(FT);, SC:M;RV:M;RF:U;EI:U;SP:U;SU:U;, P0123 , S123, R765, D123,0, ORIGINAL,,, CONFIRMED, pub/AEP/incoming,, 20000422160723ES, 20000422171523ES, Bid price refused,, Negotiated OFFER_PRICE accepted,, Joe Smith, (888)-123-4567, (888)-123-1231, jsmith@xyz.com, Jane Doe, (999)-123-4567, (999)-123-8823,,7019,20, 20000423040000ES, 20000423080000ES(
Y,8236,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,7880,10, 20000423080000ES, 20000423160000ES(
Y,8236,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,7019,10, 20000423080000ES, 20000423160000ES(
011-4.6
Examples of Negotiation of Price and Partial Service Offer

011-4.6.1
Negotiation with Preconfirmation

a. The Customer submits a PRECONFIRMED transmission service request using the transrequest Template. Initially, the STATUS is set to QUEUED by the OASIS Node. 
b. The Seller has the option of setting STATUS via the transsell Template to one of the following: INVALID, RECEIVED, STUDY, COUNTEROFFER, ACCEPTED, DECLINED, or REFUSED.
c. The Seller has the option of entering a CAPACITY_GRANTED and setting the STATUS to COUNTEROFFER via the transell Template if the seller can only provide partial service.
d. If the Seller sets STATUS to ACCEPTED (and, as required by Section 4.2.10.1i, the OASIS Node forces the Seller to set OFFER_PRICE equal to BID_PRICE as a condition to setting STATUS to ACCEPTED) and CAPACITY_GRANTED is equal to CAPACITY_REQUESTED, the OASIS Node will immediately set STATUS to CONFIRMED. (Section 4.2.10.1k requires the OASIS Node to set a null CAPACITY_GRANTED equal to CAPACITY_REQUESTED when STATUS is set to ACCEPTED.)
e. The Customer may WITHDRAW request via transcust Template at any time up to point where the Seller sets STATUS to ACCEPTED. 
f. Once the STATUS is CONFIRMED, the OFFER_PRICE and CAPACITY_GRANTED officially becomes the terms of the reservation.

011-4.6.2
Negotiations without Preconfirmation

a. The Customer submits a transmission reservation request with the BID_PRICE less than the CEILING_PRICE via the transrequest Template. Initially the STATUS is set to QUEUED by the OASIS Node.
b. The Seller has the option of setting the STATUS via the transsell Template to one of the following: INVALID, RECEIVED, STUDY, ACCEPTED, DECLINED, COUNTEROFFER, or REFUSED. If INVALID (due to invalid entries in the request), DECLINED (due to the Seller determining that the proposed price is not acceptable and further negotiations are not desired), or REFUSED (due to the unavailability of the requested service) are set, the transmission reservation request is terminated.
c. The Seller has the option of entering a CAPACITY_GRANTED and setting the STATUS to COUNTEROFFER via the transell Template if the seller can only provide partial service.
d. If the Seller set the STATUS to RECEIVED or STUDY, and determines that the BID_PRICE is too low, the Seller sets the OFFER_PRICE to the price desired, and sets the STATUS to COUNTEROFFER via the transsell Template. 
e. The Customer agrees to the OFFER_PRICE, sets the BID_PRICE equal to the OFFER_PRICE, and sets the STATUS to CONFIRMED via the transcust Template.
f. The OFFER_PRICE and CAPACITY_GRANTED with the STATUS of CONFIRMED locks in the terms of the reservation.

011-4.6.3
Multiple Step Negotiations

a. The Customer submits a transmission reservation request with the BID_PRICE less than the CEILING_PRICE via the transrequest Template. Initially the STATUS is set to QUEUED by the OASIS Node.
b. The Seller has the option of setting the STATUS via the transsell Template to one of the following: INVALID, RECEIVED, STUDY, ACCEPTED, DECLINED, COUNTEROFFER, or REFUSED. If INVALID, DECLINED, or REFUSED are set, the transmission reservation request is terminated.
c. The seller has the option of entering a CAPACITY_GRANTED and setting the STATUS to COUNTEROFFER via the transell Template if the seller can only provide partial service. If ATC changes before the request reaches the STATUS of CONFIRMED, seller may change the CAPACITY_GRANTED.
d. The Seller determines that the BID_PRICE is too low, sets the OFFER_PRICE to the desired value, and sets the STATUS to COUNTEROFFER via the transsell Template. 
e. The Customer responds to the new OFFER_PRICE with an updated BID_PRICE and sets the STATUS to REBID for re-evaluation by the Seller.
f. The Seller determines that the BID_PRICE now is acceptable, and sets the STATUS to ACCEPTED via the transsell Template. The transition to ACCEPTED state requires the OFFER_PRICE to be set to the BID_PRICE: accepting a reservation with an OFFER_PRICE different from BID_PRICE would require the STATUS be set to COUNTEROFFER rather than ACCEPTED (see item c).
g. The Customer agrees to the OFFER_PRICE and sets the STATUS to CONFIRM via the transcust Template.
h. The OFFER_PRICE and CAPACITY_GRANTED with the STATUS as CONFIRMED locks in the terms of the reservation.

011-4.6.4
Negotiations Declined by Seller

a. The Customer submits a transmission reservation request with the BID_PRICE less than the CEILING_PRICE via the transrequest Template. Initially the STATUS is set to QUEUED by the OASIS Node.
b. The Seller has the option of setting the STATUS via the transsell Template to one of the following: INVALID, RECEIVED, STUDY, ACCEPTED, DECLINED, COUNTEROFFER, or REFUSED. If INVALID, DECLINED, or REFUSED are set, the transmission reservation request is terminated.
c. The Seller determines that the BID_PRICE is too low, sets OFFER_PRICE to his desired value, and sets STATUS to COUNTEROFFER via the transsell Template. 
d. The Customer responds to OFFER_PRICE with updated BID_PRICE and sets the STATUS to REBID via the transcust Template for re-evaluation by Seller.
e. The Seller breaks off all further negotiations by setting the STATUS to DECLINED, indicating that the price is unacceptable and that he does not wish to continue negotiations.

011-4.6.5
Negotiations Withdrawn by Customer

a. The Customer submits a transmission reservation request with the BID_PRICE less than the CEILING_PRICE via the transrequest. Initially the STATUS is set to QUEUED by the OASIS Node.
b. The Seller has the option of setting the STATUS via the transsell Template to one of the following: INVALID, RECEIVED, STUDY, ACCEPTED, DECLINED, COUNTEROFFER, or REFUSED. If INVALID, DECLINED, or REFUSED are set, the transmission reservation request is terminated.
c. The Seller has the option of entering a CAPACITY_GRANTED and setting the STATUS to COUNTEROFFER via the transell Template if the seller can only provide partial service.
d. The Seller determines that the BID_PRICE is too low, sets the OFFER_PRICE to his desired value, and sets the STATUS to COUNTEROFFER via the transsell Template.
e. The Customer responds to the OFFER_PRICE with an updated BID_PRICE and sets the STATUS to REBID for re-evaluation by Seller.
f. The Seller determines that the BID_PRICE is still too low, sets the OFFER_PRICE to another value, and sets STATUS to COUNTEROFFER via the transsell Template.
g. The Customer breaks off all further negotiations, either because the OFFER_PRICE or CAPACITY_GRANTED are unacceptable, by setting STATUS to WITHDRAWN (or the Customer/Seller could go through additional iterations of REBID/COUNTEROFFER until negotiations are broken off or the reservation is CONFIRMED).

011-4.6.6
Negotiations Superseded by Higher Priority Reservation

a. The Customer submits a transmission reservation request with the BID_PRICE less than the CEILING_PRICE via the transrequest Template. Initially the STATUS is set to QUEUED by the OASIS Node.
b. The Seller has the option of setting the STATUS via the transsell Template to one of the following: INVALID, RECEIVED, STUDY, ACCEPTED, DECLINED, COUNTEROFFER, or REFUSED. If INVALID, DECLINED, or REFUSED are set, the transmission reservation request is terminated.
c. If the Seller determines that another reservation has higher priority and must displace this request, he sets the STATUS to SUPERSEDED and the negotiations are terminated.
d. However, if desired and permitted by the tariff, the Seller may set the STATUS of a request in any of these previous states (including COUNTEROFFER and ACCEPTED) to COUNTEROFFER with an OFFER_PRICE which could avoid the request being superseded, thus allowing the Customer the choice of being SUPERSEDED or accepting the proposed OFFER_PRICE.

011-4.7
Audit Template examples

The following examples are included to show the general type of audit report responses that could be expected to be returned by implementations of the audit reporting Templates as documented above.

011-4.7.1
Offerings

The following is an example of a hypothetical audit query for daily non-firm offerings to the "DDD" point of delivery for Monday August 17, 1998 (line breaks and indentations added to improve readability):
REQUEST_STATUS=200 (
ERROR_MESSAGE (
TIME_STAMP=19980821091601ES (
VERSION=1.4 (
TEMPLATE=transofferingaudit (
OUTPUT_FORMAT=DATA (
PRIMARY_PROVIDER_CODE=WXYZ (
PRIMARY_PROVIDER_DUNS=78912345 (
RETURN_TZ=ES (
DATA_ROWS=14 (
COLUMN_HEADERS=RECORD_TYPE,TIME_OF_LAST_UPDATE,MODIFYING_COMPANY_CODE,MODIFYIN G_NAME, TIME_OF_LAST_UPDATE,SELLER_CODE,SELLER_DUNS,PATH_NAME,POINT_OF_RECEIPT,POINT_OF_DEL IVERY, INTERFACE_TYPE,OFFER_START_TIME,OFFER_STOP_TIME,START_TIME,STOP_TIME,CAPACITY,SERVIC E_INCREMENT, TS_CLASS,TS_TYPE,TS_PERIOD,TS_WINDOW,TS_SUBCLASS,ANC_SVC_REQ,SALE_REF,POSTING_REF,CEI LING_PRICE, OFFER_PRICE,PRICE_UNITS,SERVICE_DESCRIPTION,NERC_CURTAILMENT_PRIORITY,OTHER_CURTAIL MENT_PRIORITY, SELLER_NAME,SELLER_PHONE,SELLER_FAX,SELLER_EMAIL,SELLER_COMMENTS (
U,19980815131756ES,WXYZ,Jane Doe,19980815131756ES, WXYZ,78912345,X/WXYZ/AAA-DDD//,AAA,DDD,E,19 980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,800, DAILY,NON-FIRM,POINT_TO_POINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48732,102.00,85.00,$/MW-Day,,3,, Jane Doe,123-456-7813,123-456-7801, doej@wxyz.com (
U,19980815124022ES,WXYZ, Jane Doe,19980815124022ES, WXYZ,78912345,X/WXYZ/AAA-DDD//,AAA,DDD,E, 1 9980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,850, DAILY,NON-FIRM,POINT_TO_ POINT,FULL_PERIOD,FIXED,,SC:M;RF:M,, 48732,102.00,85.00,$/MW-Day,,3,, Jane Doe,123-456-7813,123-456-780 1,doej@wxyz.com, (
U,19980814120018ES,WXYZ, Joe Smith,19980814120018ES,WXYZ,78912345,X/WXYZ/AAA-DDD//,AAA,DDD,E,1 9980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,850, DAILY,NON-FIRM,POINT_TO_ POINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48732,102.00,90.00,$/MW-Day,,3,,Joe Smith,123-456-7893,123-456-7801 ,smithj@wxyz.com (
I,19980813171204ES,WXYZ, Supervisor,19980813171204ES, WXYZ,78912345,X/WXYZ/AAA-DDD//,AAA,DDD,E, 19980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,850, DAILY,NON-FIRM,POINT_TO _POINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48732,102.00,95.00,$/MW-Day,,3,, Supervisor,123-456-7890,123-456-78 01 (
U,19980815124022ES,WXYZ, Jane Doe,19980815124022ES, WXYZ,78912345,X/WXYZ/BBB-DDD//,BBB,DDD,E,19 980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,1200, DAILY,NON-FIRM,POINT_TO_ POINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48783,102.00,85.00,$/MW-Day,,3,,Jane Doe,123-456-7813,123-456-7801, doej@wxyz.com (
U,19980814120022ES,WXYZ,Joe Smith,19980814120022ES,WXYZ,78912345,X/WXYZ/BBB-DDD//,BBB,DDD,E,19 980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,1200,DAILY,NON-FIRM,POINT_TO_ POINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48783,102.00,90.00,$/MW-Day,,3,,Joe Smith,123-456-7893,123-456-7801 ,smithj@wxyz.com (
I,19980813171210ES,WXYZ,Supervisor,19980813171210ES,WXYZ,78912345,X/WXYZ/BBB-DDD//,BBB,DDD,E,19 980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,1200,DAILY,NON-FIRM,POINT_TO_ POINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48783,102.00,95.00,$/MW-Day,,3,,Supervisor,123-456-7890,123-456-780 1, (
U,19980816101000ES,WXYZ,Supervisor,19980816101000ES,WXYZ,78912345,X/WXYZ/CCC-DDD//,CCC,DDD,E,19 980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,85,DAILY,NON-FIRM,POINT_TO_PO INT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48820,102.00,102.00,$/MW-Day,,3,,Supervisor,123-456-7810,123-456-7801, 5U,19980814143807ES,WXYZ,Supervisor,19980814143807ES,WXYZ,78912345,X/WXYZ/CCC-DDD//,CCC,DDD,E,19 980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,90,DAILY,NON-FIRM,POINT_TO_PO INT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48820,102.00,102.00,$/MW-Day,,3,,Supervisor,123-456-7890,123-456-7801, 5U,19980814120023ES,WXYZ,Joe Smith,19980814120023ES,WXYZ,78912345,X/WXYZ/CCC-DDD//,CCC,DDD,E,19 980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,110,DAILY,NON-FIRM,POINT_TO_P OINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48820,102.00,90.00,$/MW-Day,,3,,Joe Smith,123-456-7893,123-456-7801,s mithj@wxyz.com (
I,19980813171214ES,WXYZ,Supervisor,19980813171214ES,WXYZ,78912345,X/WXYZ/CCC-DDD//,CCC,DDD,E,19 980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,110,DAILY,NON-FIRM,POINT_TO_P OINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48820,102.00,95.00,$/MW-Day,,3,,Supervisor,123-456-7890,123-456-7801, (
U,19980815124023ES,WXYZ,Jane Doe,19980815124023ES,WXYZ,78912345,X/WXYZ/WXYZ-DDD//,WXYZ,DDD, E,19980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,340,DAILY,NON-FIRM,POINT_T O_POINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48855,102.00,85.00,$/MW-Day,,3,,Jane Doe,123-456-7813,123-456-78 01,doej@wxyz.com (
U,19980814120023ES,WXYZ,Joe Smith,19980814120023ES,WXYZ,78912345,X/WXYZ/WXYZ-DDD//,WXYZ,DDD, E,19980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,340,DAILY,NON-FIRM,POINT_T O_POINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48855,102.00,90.00,$/MW-Day,,3,,Joe Smith,123-456-7893,123-456-7 801,smithj@wxyz.com (
I,19980813171222ES,WXYZ,Supervisor,19980813171222ES,WXYZ,78912345,X/WXYZ/WXYZ-DDD//,WXYZ,DDD, E,19980814000000ES,19980817000000ES,19980817000000ES,19980818000000ES,340, DAILY,NON-FIRM,POINT_T O_POINT,FULL_PERIOD,FIXED,,SC:M;RF:M,,48855,102.00,95.00,$/MW-Day,,3,,Supervisor,123-456-7890,123-456-7 801, (
From this audit report, the daily non-firm offerings on the four paths to "DDD" (AAA-DDD, BBB-DDD, CCC-DDD, and WXYZ-DDD) were all originally posted by WXYZ's "Supervisor" at approximately 17:12 on 8/13 at a price of $95.00 /MW-Day discounted from a ceiling price of $102.00.

At approximately 12:00 on 8/14, Joe Smith changed the offer price to $90.00 on all four paths.
At 14:14 on 8/14, "Supervisor" adjusted the capacity available on path X/WXYZ/CCC-DDD// to 90 MW (POSTING_REF = 48820) and set the offer price up to match the tariff ceiling rate (presumably due to the path now being constrained and released from the requirement to have discounted service offered at the same rate as all other unconstrained paths to DDD). Capacity on this path was last updated to a value of 85 MW at 10:10 on 8/16, which is the current information posted on OASIS for this path at the time of the query.
Jane Doe adjusted the price on the three presumably unconstrained paths to DDD at 12:40 on 8/15 to $85.00, which may have been in response to a negotiation for service on one of these paths. No further updates have occurred to the offerings on paths BBB-DDD and WXYZ-DDD since that time.
Finally, the capacity available on path X/WXYZ/AAA-DDD// was updated by Jane Doe from 850 to 800 MW at 13:17 on 8/15, which may have corresponded with final confirmation of a reservation at a negotiated discount by the customer that initiated the price change from $90.00 to $85.00.

011-4.7.2
Reservations

The following is an example of a hypothetical audit query for a specific transmission service reservation (line breaks and indentations added to improve readability):
REQUEST_STATUS=200(
ERROR_MESSAGE=(
TIME_STAMP=19980821092048ES(
VERSION=1.4(
TEMPLATE=transstatusaudit(
OUTPUT_FORMAT=DATA(
PRIMARY_PROVIDER_CODE=WXYZ(
PRIMARY_PROVIDER_DUNS=78912345(
RETURN_TZ=ES(
DATA_ROWS=9(
COLUMN_HEADERS=RECORD_TYPE,TIME_OF_UPDATE,MODIFYING_COMPANY_CODE,MODIFYING_NAME, CONTINUATION_FLAG,ASSIGNMENT_REF,SELLER_CODE,SELLER_DUNS,CUSTOMER_CODE, CUSTOMER_DUNS,AFFILIATE_FLAG,PATH_NAME,POINT_OF_RECEIPT,POINT_OF_DELIVERY, SOURCE,SINK,CAPACITY,SERVICE_INCREMENT,TS_CLASS,TS_TYPE,TS_PERIOD,TS_WINDOW, TS_SUBCLASS,NERC_CURTAILMENT_PRIORITY,OTHER_CURTAILMENT_PRIORITY,START_TIME, STOP_TIME,CEILING_PRICE,OFFER_PRICE,BID_PRICE,PRICE_UNITS,PRECONFIRMED,ANC_SVC_LINK,ANC _SVC_REQ,POSTING_REF,SALE_REF,REQUEST_REF,DEAL_REF,NEGOTIATED_PRICE_FLAG, STATUS,STATUS_NOTIFICATION,STATUS_COMMENTS,TIME_QUEUED,RESPONSE_TIME_LIMIT, TIME_OF_LAST_UPDATE,PRIMARY_PROVIDER_COMMENTS,SELLER_COMMENTS, CUSTOMER_COMMENTS,SELLER_NAME,SELLER_PHONE,SELLER_FAX,SELLER_EMAIL, CUSTOMER_NAME,CUSTOMER_PHONE,CUSTOMER_FAX,CUSTOMER_EMAIL,REASSIGNED_REF, REASSIGNED_CAPACITY, REASSIGNED_START_TIME,REASSIGNED_STOP_TIME(
U,19980815131629ES,DEFPM,Alan Trader,N,104392,WXYZ,78912345,DEFPM,912876543,N,X/WXYZ/AAA-DDD//,A AA,DDD,AAA,ZZZ,50,DAILY,NON-FIRM,POINT_TO_POINT,FULL_PERIOD,FIXED,,3,,19980817000000ES,199808 18000000ES,102.00,85.00,85.00,$/MW-Day,N,,SC:M;RF:M,,,,,,CONFIRMED,,,19980815121510ES,19980815144100ES, 19980815131629ES,,,,Jane Doe,123-456-7813,123-456-7801,doej@wxyz.com,Alan Trader,312-678-9104,312-678-9100,a .trader@defmarketing.com,,,, (
U,,,,Y,,,,,,,,,,,,75,,,,,,,,,19980818000000ES,19980819000000ES,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,, (
U,,,,Y,,,,,,,,,,,,100,,,,,,,,,19980819000000ES,19980820000000ES,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,, (
U,19980815125042ES,WXYZ,Jane Doe,N,104392,WXYZ,78912345,DEFPM,912876543,N,X/WXYZ/AAA-DDD//,AAA ,DDD,AAA,ZZZ,50,DAILY,NON-FIRM,POINT_TO_POINT,FULL_PERIOD,FIXED,,3,,19980817000000ES,19980818 000000ES,102.00,85.00,82.00,$/MW-Day,N,,SC:M;RF:M,,,,,,COUNTEROFFER,,,19980815121510ES,19980815144100 ES,19980815125042ES,,,,Jane Doe,123-456-7813,123-456-7801,doej@wxyz.com,Alan Trader,312-678-9104,312-678-910 0,a.trader@defmarketing.com,,,, (
U,19980815124811ES,DEFPM,Alan Trader,N,104392,WXYZ,78912345,DEFPM,912876543,N,X/WXYZ/AAA-DDD//,A AA,DDD,AAA,ZZZ,50,DAILY,NON-FIRM,POINT_TO_POINT,FULL_PERIOD,FIXED,,3,,19980817000000ES,199808 18000000ES,102.00,85.00,82.00,$/MW-Day,N,,SC:M;RF:M,,,,,,REBID,,,19980815121510ES,19980815144100ES,19980 815124811ES,,,,Jane Doe,123-456-7813,123-456-7801,doej@wxyz.com,Alan Trader,312-678-9104,312-678-9100,a.trader @defmarketing.com(
U,19980815124100ES,WXYZ,Jane Doe,N,104392,WXYZ,78912345,DEFPM,912876543,N,X/WXYZ/AAA-DDD//,AAA ,DDD,AAA,ZZZ,50,DAILY,NON-FIRM,POINT_TO_POINT,FULL_PERIOD,FIXED,,3,,19980817000000ES,19980818 000000ES,102.00,85.00,80.00,$/MW-Day,N,,SC:M;RF:M,,,,,,COUNTEROFFER,,,19980815121510ES,19980815144100 ES,19980815124100ES,,,,Jane Doe,123-456-7813,123-456-7801,doej@wxyz.com,Alan Trader,312-678-9104,312-678-910 0,a.trader@defmarketing.com(
I,19980815121510ES,DEFPM,Alan Trader,N,104392,WXYZ,78912345,DEFPM,912876543,N,X/WXYZ/AAA-DDD//,A AA,DDD,AAA,ZZZ,50,DAILY,NON-FIRM,POINT_TO_POINT,FULL_PERIOD,FIXED,,3,,19980817000000ES,199808 18000000ES,102.00,90.00,80.00,$/MW-Day,N,,SC:M;RF:M,,,,,,QUEUED,,,19980815121510ES,,19980815121510ES,,,,Company Default,123-456-7800,123-456-7801,,Alan Trader,312-678-9104,312-678-9100,a.trader@defmarketing.com(
I,,,,Y,,,,,,,,,,,,75,,,,,,,,,19980818000000ES,19980819000000ES,,,,,,,,,,,,,,,,,,,,,,,,,,,,, (
I,,,,Y,,,,,,,,,,,,100,,,,,,,,,19980819000000ES,19980820000000ES,,,,,,,,,,,,,,,,,,,,,,,,,,,,, (
First, this example shows the handling of continuation records which conveyed a time varying demand of 50 MW on 8/17, 75 MW on 8/18, and 100 MW on 8/19. This demand profile was initially entered with the original reservation request (transrequest Template) at 12:15 on 8/15 by Alan Trader. Since the Data Elements associated with the profile were never modified, the intervening audit response records do not repeat the data from these continuation records.
As part of the original reservation, Alan Trader attempted to negotiate a price for service of $80.00 /MW-Day. Jane Doe responded to this request with a counter offer at the rate of $85.00 /MW-Day at 12:41 on 8/15. Since the status of COUNTEROFFER constitutes acceptance of all terms of the reservation except price (i.e., transmission capability has been evaluated and is available), the RESPONSE_TIME_LIMIT Data Element has been updated to reflect the time by which the customer must confirm service (assuming the establishment of customer confirmation time limits is approved by FERC). 
At 12:48, Alan Trader attempted to negotiate further for a rate of $82.00 /MWDay and the reservation status was set to REBID. Jane Doe responded at 12:50 with a second counter offer restating a rate of $85.00, which Alan Trader finally agreed to at 13:16 on 8/15. The current posted information on OASIS shows this final CONFIRMED reservation.




























































































































































































































































































































































































































































































































































































































































�This is a new concept for DEFERRAL.  Not sure if many would want to add this feature which is why I set it to “may” as an option.  If its made a requirement, we should have a companion business practice related to its use in this manner.
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