867 Product Transfer and Resale Report - MSIN

Functional Group ID=PT

Heading:

	Pos.	Seg.		Req.		Loop	
	No.	ID	Name	Des.	Max.Use	Repeat		
Must Use	0100	ST	Transaction Set Header	M	1									
Must Use	0200	BPT	Beginning Segment for Product Transfer and Resale	M	1									
	0500	DTM	Date/Time Reference	O	10									
			LOOP ID - N1			>1								
	0800	N1	Party Identification	O	1									
			LOOP ID - PER			>1								
	1300	PER	Administrative Communications Contact	O	1									

Detail:

	Pos.	Seg.		Req.		Loop	
	No.	ID	Name	Des.	Max.Use	Repeat		
			LOOP ID - PTD			>1								
Must Use	0100	PTD	Product Transfer and Resale Detail	M	1									
	0300	REF	Reference Information	O	20									
Must Use	0475	LCD	Place/Location Description	O	2									
Must Use	0490	LQ	Industry Code Identification	O	>1									
			LOOP ID - QTY			>1								
Must Use	1100	QTY	Quantity Information	O	1									
	1600	MEA	Measurements	O	40									
	2100	DTM	Date/Time Reference	O	10									
			LOOP ID - LM			>1								
Must Use	2600	LM	Code Source Information	O	1									
	2700	LQ	Industry Code Identification	O	100									

Summary:

	Pos.	Seg.		Req.		Loop	
	No.	ID	Name	Des.	Max.Use	Repeat		
Must Use	0300	SE	Transaction Set Trailer	M	1									

	Segment:	ST Transaction Set Header
	Position:	0100
	Loop:
	Level:	Heading
	Usage:	Mandatory
	Max Use:	1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	ST01	143	Transaction Set Identifier Code	M	1 	ID 3/3	
 	867		Product Transfer and Resale Report	
Must Use	ST02	329	Transaction Set Control Number	M	1 	AN 4/9	

	Segment:	BPT Beginning Segment for Product Transfer and Resale
	Position:	0200
	Loop:
	Level:	Heading
	Usage:	Mandatory
	Max Use:	1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	BPT01	353	Transaction Set Purpose Code	M	1 	ID 2/2	
 	00		Original	
Must Use	BPT03	373	Date	M	1 	DT 8/8	
	The date the statement was generated.	
	BPT04	755	Report Type Code	O	1 	ID 2/2	
 	MV		Metered Volumes	

	Segment:	DTM Date/Time Reference
	Position:	0500
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	10
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	DTM01	374	Date/Time Qualifier	M	1 	ID 3/3	
 	102		Issue	
 	582		Report Period	
Must Use	DTM05	1250	Date Time Period Format Qualifier	X	1 	ID 2/3	
 	CM		Date in Format CCYYMM	
 	DT		Date and Time Expressed in Format CCYYMMDDHHMM	
Must Use	DTM06	1251	Date Time Period	X	1 	AN 1/35	
	Statement Date/Time, Accounting Period 	

	Segment:	N1 Party Identification
	Position:	0800
	Loop:	N1        Optional
	Level:	Heading
	Usage:	Optional
	Max Use:	1
Notes:		For NAESB WGQ, this segment should occur once for each value in the N101 element.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	N101	98	Entity Identifier Code	M	1 	ID 2/3	
 	40		Receiver	
	Statement Recipient ID	
 	41		Submitter	
	Preparer ID	
Must Use	N103	66	Identification Code Qualifier	X	1 	ID 1/2	
 	1		D-U-N-S Number, Dun & Bradstreet	
	For NAESB WGQ, this code value may only be used when sending the Statement Recipient ID or Preparer ID.	
 	SV		Service Provider Number	
	For NAESB WGQ, this code value may only be used when sending the Statement Recipient ID Proprietary Code or Preparer ID Proprietary Code.	
Must Use	N104	67	Identification Code	X	1 	AN 2/17	
	Statement Recipient ID / Statement Recipient ID Proprietary Code, Preparer ID / Preparer ID Proprietary Code

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	

	Segment:	PER Administrative Communications Contact
	Position:	1300
	Loop:	PER        Optional
	Level:	Heading
	Usage:	Optional
	Max Use:	1
Notes:		For NAESB WGQ, this segment may only be used in the N1 loop for the Preparer ID (N101 = '41').	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	PER01	366	Contact Function Code	M	1 	ID 2/2	
 	IC		Information Contact	
Must Use	PER02	93	Name	O	1 	AN 1/35	
	Contact Person (Name) 

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	
Must Use	PER03	365	Communication Number Qualifier	X	1 	ID 2/2	
 	TE		Telephone	
Must Use	PER04	364	Communication Number	X	1 	AN 1/80	
	Contact Person (Phone) 

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	

	Segment:	PTD Product Transfer and Resale Detail
	Position:	0100
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Mandatory
	Max Use:	1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	PTD01	521	Product Transfer Type Code	M	1 	ID 2/2	
 	FG		Flowing Gas Information	

	Segment:	REF Reference Information
	Position:	0300
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	20
Notes:		For NAESB WGQ, this segment is sender's option.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	REF01	128	Reference Identification Qualifier	M	1 	ID 2/3	
 	ZZ		Mutually Defined	
Must Use	REF02	127	Reference Identification	X	1 	AN 1/30	
	Meter ID Relationship 
          ADD - Additive
          DED - Deductive

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	

	Segment:	LCD Place/Location Description
	Position:	0475
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional (Must Use)
	Max Use:	2
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	LCD02	98	Entity Identifier Code	O	1 	ID 2/3	
 	LCN		Gas Nomination Location	
 	MTR		Meter Location	
Must Use	LCD05	66	Identification Code Qualifier	X	1 	ID 1/2	
	When a Transportation Service Provider's proprietary code is employed pursuant to this standard, the parties agree that nominations, confirmations, scheduled quantities, and capacity release documents employing such code should be for one gas day at a time, and used only until there is a verified common code for the point associated with the proprietary location code. This would include daily nominations over a weekend. Within two months following the availability of the location the parties should employ the common code and no longer employ the proprietary code for identifying such location in the datasets related to the identified standards.	
 	DR		Gas Industry Standards Board (GISB) Data Reference Number (DRN)	
	For NAESB WGQ, this code value may only be used when sending the Location Code.	
 	SV		Service Provider Number	
	For NAESB WGQ, this code value may only be used when sending the Location Proprietary Code or the Meter ID.	
Must Use	LCD06	67	Identification Code	X	1 	AN 2/17	
	Location Code / Location Proprietary Code, Meter ID 

For NAESB WGQ, Meter Id is sender's option.

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.

	Segment:	LQ Industry Code Identification
	Position:	0490
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional (Must Use)
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	LQ01	1270	Code List Qualifier Code	O	1 	ID 1/3	
 	SMB		Statement Basis	
Must Use	LQ02	1271	Industry Code	X	1 	AN 1/30	
	Statement Basis
          AC     Actual
          ES      Estimate
          RV      Revision

	Segment:	QTY Quantity Information
	Position:	1100
	Loop:	QTY        Optional (Must Use)
	Level:	Detail
	Usage:	Optional (Must Use)
	Max Use:	1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	QTY01	673	Quantity Qualifier	M	1 	ID 2/2	
 	OB		Energy	
Must Use	QTY02	380	Quantity	X	1 	R 1/15	
	Energy Quantity 	

	Segment:	MEA Measurements
	Position:	1600
	Loop:	QTY        Optional (Must Use)
	Level:	Detail
	Usage:	Optional
	Max Use:	40
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	MEA03	739	Measurement Value	X	1 	R 1/10	
	Measured Volume 

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	
Must Use	MEA04	C001	Composite Unit of Measure	X	1 		
Must Use	C00101	355	Unit or Basis for Measurement Code	M		ID 2/2	
 	TZ		Thousand Cubic Feet	

	Segment:	DTM Date/Time Reference
	Position:	2100
	Loop:	QTY        Optional (Must Use)
	Level:	Detail
	Usage:	Optional
	Max Use:	10
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	DTM01	374	Date/Time Qualifier	M	1 	ID 3/3	
 	405		Production	
Must Use	DTM05	1250	Date Time Period Format Qualifier	X	1 	ID 2/3	
 	RD8		Range of Dates Expressed in Format CCYYMMDD-CCYYMMDD	
	This code designates the range of "gas days" in which the transaction will occur. For example, the entire month of April 2001 would be stated as 20010401-20010430.	
 	RDT		Range of Date and Time, Expressed in Format CCYYMMDDHHMM-CCYYMMDDHHMM	
	This code designates the instance in time when the transaction is to be initiated through the instance in time when the transaction is to finish. For example, the entire month of April 2001 would be stated as 200104010900-200105010900.	
Must Use	DTM06	1251	Date Time Period	X	1 	AN 1/35	
	Beginning Flow Date, Beginning Flow Time, Ending Flow Date, Ending Flow Time	

	Segment:	LM Code Source Information
	Position:	2600
	Loop:	LM        Optional (Must Use)
	Level:	Detail
	Usage:	Optional (Must Use)
	Max Use:	1
Notes:		For NAESB WGQ, this segment is conditional.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	LM01	559	Agency Qualifier Code	M	1 	ID 2/2	
 	GI		Gas Industry Standards Board	

	Segment:	LQ Industry Code Identification
	Position:	2700
	Loop:	LM        Optional (Must Use)
	Level:	Detail
	Usage:	Optional
	Max Use:	100
Notes:		For NAESB WGQ, this segment is conditional.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	LQ01	1270	Code List Qualifier Code	O	1 	ID 1/3	
 	AJT		Adjustment Type	
Must Use	LQ02	1271	Industry Code	X	1 	AN 1/30	
	Adjustment Type
    ARN    Audit Review-No Adjustment Necessary
    BEQ    Heating Factor and Volume Correction
    DEE    Data Entry Error
    ECF    EFM Communication Failure
    EQC   Heating Factor Correction
    ERA   Estimate Replaced with Actual: Late
    ICA    Incorrect Chromatograph Assignment/Data
    ICT    Invalid Calculation Type
    IEC    Incorrect EFM Station Configuration
    IGQ   Incorrect Gas Quality
    IGS    Invalid Gas Sample
    IPI     Integration/Scan Process Incorrect
    LNS    Late Notification of Station Turn On
    MCN   Measured Change Not Received
    MEF   Mechanical Field Equipment Failure
    MNV   Missing Data, No Volume Estimate
    MVC   Volume Correction
    QRL   Quality Data Received Late
    VEN   Volume Estimate-No Data Received	

	Segment:	SE Transaction Set Trailer
	Position:	0300
	Loop:
	Level:	Summary
	Usage:	Mandatory
	Max Use:	1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	SE01	96	Number of Included Segments	M	1 	N0 1/10	
Must Use	SE02	329	Transaction Set Control Number	M	1 	AN 4/9