873 Commodity Movement Services

Functional Group ID=CU

Heading:

	Pos.	Seg.		Req.		Loop	
	No.	ID	Name	Des.	Max.Use	Repeat		
Must Use	0100	ST	Transaction Set Header	M	1									
Must Use	0200	BGN	Beginning Segment	M	1									
	0400	DTM	Date/Time Reference	O	>1									
			LOOP ID - N1			>1								
Must Use	0500	N1	Party Identification	M	1									
	0900	PER	Administrative Communications Contact	O	3									

Detail:

	Pos.	Seg.		Req.		Loop	
	No.	ID	Name	Des.	Max.Use	Repeat		
			LOOP ID - DTM			>1								
Must Use	0100	DTM	Date/Time Reference	M	1									
	0200	N9	Extended Reference Information	O	>1									
	0300	LQ	Industry Code Identification	O	>1									
	0400	LCD	Place/Location Description	O	1									
			LOOP ID - SLN			>1								
	0700	SLN	Subline Item Detail	O	1									
	0800	LQ	Industry Code Identification	O	>1									
	0900	N9	Extended Reference Information	O	>1									
	1000	QTY	Quantity Information	O	>1									
			LOOP ID - N1			>1								
	1100	N1	Party Identification	O	1									
	1200	LCD	Place/Location Description	O	1									
	1300	N9	Extended Reference Information	O	>1									
														
Must Use	1600	SE	Transaction Set Trailer	M	1									

	Segment:	ST Transaction Set Header
	Position:	0100
	Loop:
	Level:	Heading
	Usage:	Mandatory
	Max Use:	1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	ST01	143	Transaction Set Identifier Code	M	1 	ID 3/3	
 	873		Commodity Movement Services	
Must Use	ST02	329	Transaction Set Control Number	M	1 	AN 4/9	

	Segment:	BGN Beginning Segment
	Position:	0200
	Loop:
	Level:	Heading
	Usage:	Mandatory
	Max Use:	1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	BGN01	353	Transaction Set Purpose Code	M	1 	ID 2/2	
 	00		Original	
Must Use	BGN02	127	Reference Identification	M	1 	AN 1/22	
	The PDA number assigned by the PDA originator.

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	
Must Use	BGN03	373	Date	M	1 	DT 8/8	
	The PDA issue date.	
Must Use	BGN07	640	Transaction Type Code	O	1 	ID 2/2	
 	F4		Pre-determined Allocation	

	Segment:	DTM Date/Time Reference
	Position:	0400
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	DTM01	374	Date/Time Qualifier	M	1 	ID 3/3	
 	102		Issue	
Must Use	DTM05	1250	Date Time Period Format Qualifier	X	1 	ID 2/3	
 	DT		Date and Time Expressed in Format CCYYMMDDHHMM	
Must Use	DTM06	1251	Date Time Period	X	1 	AN 1/35	
	Statement Date/Time 	

	Segment:	N1 Party Identification
	Position:	0500
	Loop:	N1        Mandatory
	Level:	Heading
	Usage:	Mandatory
	Max Use:	1
Notes:		For NAESB WGQ, this segment is mandatory and should occur once for each value in the N101 element.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	N101	98	Entity Identifier Code	M	1 	ID 2/3	
 	40		Receiver	
	Statement Recipient ID	
 	41		Submitter	
	Preparer ID 	
Must Use	N103	66	Identification Code Qualifier	X	1 	ID 1/2	
 	1		D-U-N-S Number, Dun & Bradstreet	
 	SV		Service Provider Number	
Must Use	N104	67	Identification Code	X	1 	AN 2/17	
	Statement Recipient ID / Statement Recipient ID Proprietary Code, Preparer ID / Preparer ID Proprietary Code

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	

	Segment:	PER Administrative Communications Contact
	Position:	0900
	Loop:	N1        Mandatory
	Level:	Heading
	Usage:	Optional
	Max Use:	3
Notes:		For NAESB WGQ, this segment may only be used in the N1 loop for the Preparer ID (N101 = '41').	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	PER01	366	Contact Function Code	M	1 	ID 2/2	
 	IC		Information Contact	
Must Use	PER02	93	Name	O	1 	AN 1/35	
	Contact Person (Name) 

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	
Must Use	PER03	365	Communication Number Qualifier	X	1 	ID 2/2	
 	TE		Telephone	
Must Use	PER04	364	Communication Number	X	1 	AN 1/80	
	Contact Person (Phone) 

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.

	Segment:	DTM Date/Time Reference
	Position:	0100
	Loop:	DTM        Mandatory
	Level:	Detail
	Usage:	Mandatory
	Max Use:	1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	DTM01	374	Date/Time Qualifier	M	1 	ID 3/3	
 	405		Production	
Must Use	DTM05	1250	Date Time Period Format Qualifier	X	1 	ID 2/3	
 	RD8		Range of Dates Expressed in Format CCYYMMDD-CCYYMMDD	
	This code designates the first "gas day" through the last "gas day" in which gas will flow. Example: For a gas day beginning and ending at 9:00am, the entire month of April 1996 would be stated 19960401-19960430 	
 	RDT		Range of Date and Time, Expressed in Format CCYYMMDDHHMM-CCYYMMDDHHMM	
	This code designates the instance in time when the gas will begin to flow through the instance in time when the gas will cease to flow. Example: For a gas day beginning and ending at 9:00am, the entire month of April 1996 would be stated 199604010900-199605010900	
Must Use	DTM06	1251	Date Time Period	X	1 	AN 1/35	
	Beginning Flow Date, Beginning Flow Time, Ending Flow Date, Ending Flow Time

	Segment:	N9 Extended Reference Information
	Position:	0200
	Loop:	DTM        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	N901	128	Reference Identification Qualifier	M	1 	ID 2/3	
 	06		System Number	
Must Use	N902	127	Reference Identification	X	1 	AN 1/11	
	assigned identification

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	

	Segment:	LQ Industry Code Identification
	Position:	0300
	Loop:	DTM        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	LQ01	1270	Code List Qualifier Code	O	1 	ID 1/3	
	Refer to "LQ Segments (Detail)" table for usage and values.	
Must Use	LQ02	1271	Industry Code	X	1 	AN 1/30	
	Direction of Flow, Pre-determined Allocation (PDA) Transaction Type Code

Refer to "LQ Segments (Detail)" table for usage and values.	

	Segment:	LCD Place/Location Description
	Position:	0400
	Loop:	DTM        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	1
Notes:		For NAESB WGQ, this segment is mandatory	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	LCD02	98	Entity Identifier Code	O	1 	ID 2/3	
 	LCN		Gas Nomination Location	
Must Use	LCD05	66	Identification Code Qualifier	X	1 	ID 1/2	
	When a Transportation Service Provider's proprietary code is employed pursuant to this standard, the parties agree that nominations, confirmations, scheduled quantities, and capacity release documents employing such code should be for one gas day at a time, and used only until there is a verified common code for the point associated with the proprietary location code. This would include daily nominations over a weekend. Within two months following the availability of the location the parties should employ the common code and no longer employ the proprietary code for identifying such location in the datasets related to the identified standards.	
 	DR		Gas Industry Standards Board (GISB) Data Reference Number (DRN)	
	For NAESB, this code value may only be used when sending the Location.	
 	SV		Service Provider Number	
	For NAESB, this code value may only be used when sending the Location Proprietary Code.	
Must Use	LCD06	67	Identification Code	X	1 	AN 2/17	
	Location/Location Proprietary Code

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	

	Segment:	SLN Subline Item Detail
	Position:	0700
	Loop:	SLN        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	1
Notes:		For NAESB WGQ, this segment is mandatory	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	SLN01	350	Assigned Identification	M	1 	AN 1/11	
	PDA Submitter's Tracking ID 	
Must Use	SLN03	662	Relationship Code	M	1 	ID 1/1	
 	I		Included	
	SLN06	212	Unit Price	X	1 	R 1/14	
	For NAESB WGQ, this element is conditional

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	

	Segment:	LQ Industry Code Identification
	Position:	0800
	Loop:	SLN        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	LQ01	1270	Code List Qualifier Code	O	1 	ID 1/3	
	Refer to "LQ Segments (Sub-detail)" table for usage and values.	
	LQ02	1271	Industry Code	X	1 	AN 1/30	
	Allocation Method, Allocation Rank Indicator, Allocation Rank Level, Transaction Type, Limit Type, Swing Fuel Option Indicator

Refer to "LQ Segments (Sub-detail)" table for usage and values.	

	Segment:	N9 Extended Reference Information
	Position:	0900
	Loop:	SLN        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is conditional.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	N901	128	Reference Identification Qualifier	M	1 	ID 2/3	
 	BE		Business Activity	
	Service Provider's Activity Code 	
 	KAS		Associated Contract Identifier	
 	PKG		Package Identifier	
Must Use	N902	127	Reference Identification	X	1 	AN 1/30	
	Package ID, Service Provider's Activity Code, Associated Contract

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	

	Segment:	QTY Quantity Information
	Position:	1000
	Loop:	SLN        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is business conditional.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	QTY01	673	Quantity Qualifier	M	1 	ID 2/2	
 	LD		Limit Value	
	QTY02	380	Quantity	X	1 	R 1/15	
	Limit Value 	
	QTY03	C001	Composite Unit of Measure	O	1 		
Must Use	C00101	355	Unit or Basis for Measurement Code	M		ID 2/2	
 	BZ		Million BTU's	
 	G8		Gigacalories	
 	GV		Gigajoules	

	Segment:	N1 Party Identification
	Position:	1100
	Loop:	N1        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	1
Notes:		For NAESB WGQ, this segment is conditional based upon the usage as defined by the PDA Transaction Type Matrix	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	N101	98	Entity Identifier Code	M	1 	ID 2/3	
 	78		Service Requester	
 	DW		Downstream Party	
 	US		Upstream Party	
Must Use	N103	66	Identification Code Qualifier	X	1 	ID 1/2	
	Parties should mutually agree to use the Transportation Service Provider's proprietary entity code when the D-U-N-S® Number is not available.	
 	1		D-U-N-S Number, Dun & Bradstreet	
	For NAESB WGQ, this code value may only be used when sending the Service Requester ID, Upstream Identifier Code, Downstream Identifier Code.	
 	SV		Service Provider Number	
	For NAESB WGQ, this code value may only be used when sending the Service Requester Proprietary Code, Upstream Identifier Proprietary Code, or Downstream Identifier Proprietary Code.	
Must Use	N104	67	Identification Code	X	1 	AN 2/17	
	Service Requester ID / Service Requester Proprietary Code, Upstream Identifier Code / Upstream Identifier Proprietary Code, Downstream Identifier Code / Downstream Identifier Proprietary Code

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	

	Segment:	LCD Place/Location Description
	Position:	1200
	Loop:	N1        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	1
Notes:		For NAESB WGQ, this segment is conditional based upon the PDA Transaction Type Matrix.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
	LCD02	98	Entity Identifier Code	O	1 	ID 2/3	
 	M2		Receipt Location	
	For NAESB WGQ, this code value may only be used in the upstream N1 loop (N101 = 'US').	
 	MQ		Delivery Location	
	For NAESB WGQ, this code value may only be used in the downstream N1 loop (N101 = 'DW').	
Must Use	LCD05	66	Identification Code Qualifier	X	1 	ID 1/2	
	When a Transportation Service Provider's proprietary code is employed pursuant to this standard, the parties agree that nominations, confirmations, scheduled quantities, and capacity release documents employing such code should be for one gas day at a time, and used only until there is a verified common code for the point associated with the proprietary location code. This would include daily nominations over a weekend. Within two months following the availability of the location the parties should employ the common code and no longer employ the proprietary code for identifying such location in the datasets related to the identified standards.	
 	DR		Gas Industry Standards Board (GISB) Data Reference Number (DRN)	
	For NAESB WGQ, this code value may only be used when sending the Receipt Location or Delivery Location.	
 	SV		Service Provider Number	
	For NAESB WGQ, this code value may only be used when sending the Receipt Location Proprietary Code or Delivery Location Proprietary Code.	
Must Use	LCD06	67	Identification Code	X	1 	AN 2/17	
	Receipt Location/Receipt Location Proprietary Code, Delivery Location/Delivery Location Proprietary Code

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards	

	Segment:	N9 Extended Reference Information
	Position:	1300
	Loop:	N1        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is conditional based upon the PDA Transaction Type Matrix.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	N901	128	Reference Identification Qualifier	M	1 	ID 2/3	
 	DT		Downstream Shipper Contract Number	
	For NAESB WGQ, this code value may only be used in the downstream N1 loop (N101 = 'DW').	
 	KSR		Service Requester Contract Identifier	
	For NAESB WGQ, this code value may only be used in the service requester N1 loop (N101 = '78').	
 	PGD		Downstream Package Identifier	
	For NAESB WGQ, this code value may only be used in the downstream N1 loop (N101 = 'DW').	
 	PKU		Upstream Package Identifier	
	For NAESB WGQ, this code value may only be used in the upstream N1 loop (N101 = 'US').	
 	UP		Upstream Shipper Contract Number	
	For NAESB WGQ, this code value may only be used in the upstream N1 loop (N101 = 'US').	
Must Use	N902	127	Reference Identification	X	1 	AN 1/30	
	Downstream Contract Identifier, Downstream Package ID, Service Requester Contract, Upstream Contract Identifier, Upstream Package ID

The data element maximum length indicated is reduced from that which is specified in the ASC X12 standards.	

	Segment:	SE Transaction Set Trailer
	Position:	1600
	Loop:
	Level:	Detail
	Usage:	Mandatory
	Max Use:	1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	SE01	96	Number of Included Segments	M	1 	N0 1/10	
Must Use	SE02	329	Transaction Set Control Number	M	1 	AN 4/9