2018 API 2ai1 Template Structure

1627. “…These postings must include all circumstances and events contributing to the need for a firm service curtailment, specific services and customers curtailed (including the transmission provider’s own retail loads), and the duration of the curtailment….” (Excerpt from FERC Order 890 para 1627)

|  |  |
| --- | --- |
| Required Item | Data Element |
| Identification of the event (Firm curtailment event) | EVENT\_ID (Definition in WEQ-003 will need to be expanded to include local procedures) |
| Reason (Circumstances & events contributing) | FACILITY\_CLASS & FACILITY\_LIMIT\_TYPE & ANNOTATION & PROCEDURE\_NAME & PROCEDURE\_LEVEL |
| Services Curtailed (Transmission product & capacity) |  |
| Customers Curtailed (Entity Code) |  |
| Duration of the event | START\_TIME & STOP\_TIME (curtailment event level & sub level events as appropriate ) |